    Network Working Group                                            W. Prue
    Request for Comments:  1016                                    J. Postel
                                                                         ISI
                                                                   July 1987

                 Something a Host Could Do with Source Quench:

                   The Source Quench Introduced Delay (SQuID)

    Status of this Memo

       This memo is intended to explore the issue of what a host could do
       with a source quench.  The proposal is for each source host IP module
       to introduce some delay between datagrams sent to the same
       destination host.  This is an "crazy idea paper" and discussion is
       essential.  Distribution of this memo is unlimited.

    Introduction

       A gateway may discard Internet datagrams if it does not have the
       buffer space needed to queue the datagrams for output to the next
       network on the route to the destination network.  If a gateway
       discards a datagram, it may send a source quench message to the
       Internet source host of the datagram.  A destination host may also
       send a source quench message if datagrams arrive too fast to be
       processed.  The source quench message is a request to the host to cut
       back the rate at which it is sending traffic to the Internet
       destination.  The gateway may send a source quench message for every
       message that it discards.  On receipt of a source quench message, the
       source host should cut back the rate at which it is sending traffic
       to the specified destination until it no longer receives source
       quench messages from the gateway.  The source host can then gradually
       increase the rate at which it sends traffic to the destination until
       it again receives source quench messages [1,2].

       The gateway or host may send the source quench message when it
       approaches its capacity limit rather than waiting until the capacity
       is exceeded.  This means that the data datagram which triggered the
       source quench message may be delivered.

    The SQuID Concept

       Suppose the IP module at the datagram source has a queue of datagrams
       to send, and the IP module has a parameter "D".  D is the introduced
       delay between sending datagrams from the queue to the network.  That
       is, when the IP module discovers a datagram waiting to be sent to the
       network, it sends it to the network then waits time D before even
       looking at the datagram queue again.  Normally, the value of D is

    Prue & Postel                                                   [Page 1]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       zero.

       Imagine that when a source quench is received (or any other signal is
       received that the host should slow down its transmissions to the
       network), the value of D is increased.  As time goes by, the value of
       D is decreased.

    The SQuID Algorithm

              on increase event:

                   D <-- maximum (D + K, I)
                                            (where K = .020 second,
                                                   I = .075 second)

              on decrease event:

                   D <-- maximum (D - J, 0)
                                            (where J = .001 second)

       An increase event is receipt of one or more source quenches in a
       event period E, (where E is 2.000 seconds).

       A decrease event is when S time has passed since D was decreased and
       there is a datagram to send (where S is 1.000 seconds).

       A cache of D's is kept for the last M hosts communicated with.

       Note that when no datagrams are sent to a destination for some time
       the D for that destination is not decreased, but, if a destination is
       not used for a long time that D for that destination may fall out of
       the cache.

    Possible Refinements

       Keep a separate outgoing queue of datagrams for each destination
       host, local subnet, or network.

       Keep the cache of D's per network or local subnet, instead of per
       host.

       "I" could be based upon the basic speed of the slowest intervening
       network (see Appendix A).

       "D" could be limited to never go below "I" if the above refinement
       were implemented.

       "S" could be based upon the round trip time.

    Prue & Postel                                                   [Page 2]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       "D" could be adjusted datagram by datagram based upon the length of
       the datagrams.  Wait longer after a long datagram.

       The delay algorithm could be implemented such that if a source
       doesn't send a datagram when it is next allowed (the introduced delay
       interval) or for N such intervals that the source gets a credit for
       one and only one free (no delay) datagram.

    Implementation Ideas

       Since IP does not normally keep much state information about things,
       we want the default or idle IP to have no state about these D values.
       Since the default D value is zero, let us propose that the IP will
       keep a list of only those destinations with non zero D's.

       When the IP wants to send a datagram, it searches the D-list to see
       if the destination is noted.  If it is not, the D value is zero, so
       the IP sends the datagram at once.  If the destination is listed, the
       IP must wait D time indicated before sending that particular
       datagram.  It could look at a datagram addressed to a different
       destination, and possibly send it in the mean time.

       When the IP receives a source quench, it checks to see if the
       destination in the datagram that caused the source quench is on the
       list.  If so, it adds K to the D value.  If not, it appends the
       destination to the list with the D value set to "I".

    A Closer Look At the Problem

       Some implementations of IP send one SQ for every N datagrams they
       discard (for example, N=20) so the SQ messages will not make the
       congestion problem much worse [3].  In such situations any of the
       sources of the 20 datagrams may get the SQ not necessarily the one
       causing the most traffic.  However if a host continues to send
       datagrams at a high rate it has a high probability of receiving a SQ
       message sooner or later.  It is much like a speeder on a highway.
       Not all speeders get speeding tickets but the ones who speed most
       often or most excessively are most likely to be ticketed.  In this
       case they will get a ticket and their car may be destroyed.

       With memory becoming so inexpensive many IP nodes put an artificially
       low limit on the size of their queues so that through node delay will
       not be excessive [4].  For example, if one megabyte of data is
       buffered to be sent over a 56 kb/s line the last datagram will wait
       over 2 minutes before being sent.

       One problem with SQ is that the IP or ICMP specification does not
       have a well defined event to indicate receipt of SQ to higher level

    Prue & Postel                                                   [Page 3]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       protocols.  Therefore many TCP implementations do not get notified
       about SQ events and thus do not react to SQ.  TCP is not the only
       source of IP datagrams either.  Other protocols should also respond
       to SQ events in some appropriate way.  TCP and other protocols at
       that level should do something about a source quench, however,
       discussion of their behavior is beyond the scope of this memo.  Note
       that implementation of SQ processing at one level of protocol should
       not interfere with the behavior of higher level protocols.  This
       however, is difficult to do.

       For protocols using IP which are trying to transfer large amounts of
       data the data flow is most typically very bursty.  TCP for example,
       might send 5-10 segments into a window of 5-10 K bytes then wait for
       the acknowledgment of the data which opens the window again.  NETBLT
       as defined by RFC-998 is a rate based protocol which has parameters
       for burst size and burst rate.

       One purpose of the bursts is to allow the source computer to generate
       several datagrams at once to provide more efficient scheduling.  An
       other reason is to keep the network busy accepting data to maximize
       effective throughput in spite of a potentially large network round
       trip delay.  To send a datagram then wait for an acknowledgment is a
       simple but not efficient protocol on a large wide area network.

       The reasons for efficiencies obtained at the source node by
       generating many datagrams at once are not as applicable in an
       intermediate IP node.  Since each datagram is potentially from a
       different node they must all be treated individually.  Datagrams
       received in a burst may also overload the queue of an intermediate
       node losing datagrams and causing SQs to be generated.  If the queue
       is near a threshold and a burst comes, possibly all of the datagrams
       will be lost.  When datagrams arrive evenly spaced, less datagrams
       are likely to be lost because the inter-arrival time allows the queue
       a little time to empty out.  Therefore datagrams spaced with some
       delay between them may be better for intermediate IP nodes.

       Congestion is most likely to occur at IP nodes which are gateways
       between a slower network and a faster one.  The congestion will be in
       the send queue from the slow network to the fast network.  An SQ
       being returned to the sender will return on the faster network.  (See
       diagram below.)

    A Gateway Source Quench Concept

       In order for the SQuID algorithm to work we rely upon the gateways to
       send SQs to us to tell us how we are doing.  Because the loss of a
       single datagram affects data flow so much (see lost datagram
       discussion in Observed Results below) it would be much better for the

    Prue & Postel                                                   [Page 4]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       source IP node if it got a warning before datagrams were discarded.

       We propose gateway IP nodes start SQing before the node is flooded at
       a level we call SQ Keep (SQK) but forward the datagram.  If the queue
       level reaches a critical level, SQ Toss level (SQT), the gateway
       should toss datagrams to resolve the problem unless the datagram is
       an ICMP message.  Even ICMP messages will be tossed if the MaxQ level
       is reached.  Once the gateway starts sending SQs it should continue
       to do so until the queue level goes below a low water mark level
       (SQLW) as shown below.  This is analogous to methods some operating
       systems use to handle memory space management.

       The gateway should try to send SQ to as many of the contributors of
       the congestion as possible but only once per contributor per second
       or two.

       Source Quench Queue Levels

             +--------------+ MaxQ level
             |              |> datagrams tossed & SQed (but not ICMP msgs.)
             +--------------+ SQT level (95%)
             |              |\
             |              | > datagrams SQed but forwarded
             |              |/
             +--------------+ SQK level (70%)
             |              |\
             |              | \ datagrams SQed but forwarded if SQK level
             |              | / exceeded & SQLW or lower not yet reached
             |              |/
             +--------------+ SQLW level (50%)
             |              |\
             |              | \
             |              |  \
             |              |   \ datagrams forwarded
             |              |   /
             |              |  /
             |              | /
             |              |/
             +--------------+

    Description of the Test Model

       We needed some way of testing our algorithm and its various
       parameters.  It was important to check the interaction between IP
       with the SQuID algorithm and TCP.  We also wanted to try various
       combinations of retransmission strategy and source quench strategy
       which required control of the entire test network.  We therefore
       decided to build an Internet model.

    Prue & Postel                                                   [Page 5]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       Using this example configuration for illustration:

     _______    LAN       _______     WAN      _______     LAN      _______
    |   1   |            |   2   |            |   3   |            |   4   |
    |TCP/IP |---10 Mb/s--|  IP   |---56 kb/s--|  IP   |---10 Mb/s--|TCP/IP |
    |_______|            |_______|            |_______|            |_______|

       A program was written in C which created queues and structures to put
       on the queues representing datagrams carrying data, acknowledgments
       and SQs.  The program moved datagrams from one queue to the next
       based upon rules defined below

       A client fed the TCP in node 1 data at the rate it would accept.  The
       TCP function in node 1 would chop the data up into fixed 512 byte
       datagrams for transmission to the IP in node 1.  When the datagrams
       were given to IP for transmission, a timestamp was put on it and a
       copy of it was put on a TCP ack-wait queue (data sent but not yet
       acknowledged).  In particular TCP assumed that once it handed data to
       IP, the data was sent immediately for purposes of retransmission
       timeouts even though our algorithm has IP add delay before
       transmission.

       Each IP node had one queue in each direction (left and right).  For
       each IP in the model IP would forward datagrams at the rate of the
       communications line going to the next node.  Thus the fifth datagram
       on IP 2's queue going right would take 5 X 73 msec or 365 msec before
       it would appear at the end of IP 3's queue.  The time to process each
       datagram was considered to be less than the time it took for the data
       to be sent over the 56 kb/s lines and therefore done during those
       transmission times and not included in the model.  For the LAN
       communications this is not the case but since they were not at the
       bottleneck of the path this processing time was ignored.  However
       because LAN communications are typically shared band width, the LAN
       band width available to each IP instance was considered to be 1 Mb/s,
       a crude approximation.

       When the data arrived at node 4 the data was immediately given to the
       TCP receive function which validated the sequence number.  If the
       datagram was in sequence the datagram was turned into an ack datagram
       and sent back to the source.  An ack datagram carries no data and
       will move the right edge of the window, the window size past the just
       acked data sequence number.  The ack datagram is assumed to be 1/8 of
       the length of a data datagram and thus can be transmitted from one
       node to the next 8 times faster.  If the sequence number is less than
       expected (a retransmission due to a missed ack) then it too is turned
       into an ack.  A larger sequence number datagram is queued
       indefinitely until the missing datagrams are received.

    Prue & Postel                                                   [Page 6]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       We also modeled the gateway source quench algorithm.  When a datagram
       was put on an IP queue the number on the queue was compared to an SQ
       keep level (SQK).  If it was greater, an SQ was generated and
       returned to the sender. If it was larger than the SQ toss (SQT) level
       it was also discarded.  Once SQs were generated they would continue
       to be sent until the queue level went below SQ Low Water (SQLW) level
       which was below the original SQK level.  These percentages were
       modifiable as were many parameters.  An SQ could be lost if it
       exceeded the maximum queue size (MaxQ), but a source quench was never
       sent about tossing a source quench.

       Upon each transition from one node to the next, the datagram was
       vulnerable to datagram loss due to errors.  The loss rate could be
       set as M losses out of N datagrams sent, thus the model allowed for
       multi-datagram loss bursts or single datagram losses.  We used a
       single datagram loss rate of 1 lost datagram per 300 datagrams sent
       for much of our testing.  While this may seem low for Internet
       simulation, remember it does not include losses due to congestion.

       Some network parameters we used were a maximum queue length of 15
       datagrams per IP direction left and right.  We started sending SQ if
       the queue was 70% full, SQK level, tossed data datagrams, but not SQ
       datagrams, if 95% of the queue was reached, SQT level, and stopped
       SQing when a 50% SQLW level was reached (see above).

       We ignored additional SQs for 2 seconds after receipt of one SQ.
       This was done because some Internet nodes only send one SQ for every
       20 datagrams they discard even though our model sent SQs for every
       datagram discarded.  Other IP node may send one SQ per discarded
       packet. The SQuID algorithm needed a way to handle both types of SQ
       generation.  We therefore treated one or a burst of SQs as a single
       event and incremented our D by a larger amount than would be
       appropriate for responding individually to the multiple SQs of the
       verbose nodes.

       The simulation did not do any fragmenting of datagrams.  Silly window
       syndrome was avoided.  The model did not implement nor simulate the
       TTL (time-to-live) function.

       The model allowed for a flexible topology definition with many TCP
       source/destination pairs on host IP nodes or gateway IP nodes with
       various windows allowed.  An IP node could have any number of TCPs
       assigned to it.  Each line could have an individually set speed.  Any
       TCP could send to any other TCP.  The routing from one location to
       another was fixed.  Therefore datagrams did not arrive out of
       sequence.  However, datagrams arrived in ascending order, but not
       consecutively, on a regular basis because of datagram losses.
       Datagrams going "left" through a node did not affect the queue size,

    Prue & Postel                                                   [Page 7]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       or SQ chances, of data going "right" through the node.

       The TCP retransmission timer algorithm used an Alpha of .15 and a
       Beta of 1.5.  The test was run without the benefit of the more
       sophisticated retransmission timer algorithm proposed by Van Jacobson
       [5].

       The program would display either the queue sizes of the various IP
       nodes and the TCP under test as time passed or do a crude plot of
       various parameters of interest including SRTT, perceived round trip
       time, throughput, and the critical queue size.

       As we observed the effects of various algorithms for responding to SQ
       we adapted our model to better react to SQ.  Initial tests showed if
       we incremented slowly and decremented quickly we observed
       oscillations around the correct value but more of the time was spent
       over driving the network, thus losing datagrams, than at a value
       which helped the congestion situation.

       A significant problem is the delay between when some intermediate
       node starts dropping datagrams and sending source quenches to the
       time when the source quenches arrive at the source host and can begin
       to effect the behavior at the data source.  Because of this and the
       possibility that a IP might send only one SQ for each 20 datagrams
       lost, we decided that the increase in D per source quench should be
       substantial (for example, D should increase by 20 msec for every
       source quench), and the decrease with time should be very slow (for
       example, D should decrease 1 msec every second).  Note that this is
       the opposite behavior than suggested in an early draft by one of the
       authors.

       However, when many source quenches are received (for example, when a
       source quench is received for every datagram dropped) in a short time
       period the D value is increased excessively.  To prevent D from
       growing too large, we decided to ignore subsequent source quenches
       for a time (for example, 2 seconds) once we had increased D.

       Tests were run with only one TCP sending data to learn as much as
       possible how an unperturbed session might run.  Other test runs would
       introduce and eliminate competing traffic dynamically between other
       TCP instances on the various nodes to see how the algorithms reacted
       to changes in network load.  A potential flaw in the model is that
       the defined TCPs with open windows always tried to forward data.
       Their clients feeding them data never paused to think what they were
       going to type nor got swapped out in favor of other applications nor
       turned the session around logically to listen to the other end for
       more user commands.  In other words all of the simulated TCP sessions
       were doing file transfers.

    Prue & Postel                                                   [Page 8]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       The model was defined to allow many mixes of competing algorithms for
       responding to SQ.  It allowed comparing effective throughput between
       TCPs with small windows and large windows and those whose IP would
       introduce inter-datagram delays and those who totally ignored SQ.  It
       also allowed comparisons with various inter-datagram increment
       amounts and decrement amounts.  Because of the number of possible
       configurations and parameter combinations only a few combinations of
       parameters were tested. It is hoped they were the most appropriate
       ones upon which to concentrate.

    Observed Results

       All of our algorithms oscillate, some worse than others.

       If we put in just the right amount of introduced delay we seem to get
       the best throughput.  But finding the right amount is not easy.

       Throughput is adversely affected, heavily, by a single lost datagram
       at least for the short time.  Examine what happens when a window is
       35 datagrams wide with an average round trip delay of 2500 msec using
       512 byte datagrams when a single datagram is lost at the beginning.
       Thirty five datagrams are given by TCP to IP and a timer is started
       on the first datagram.  Since the first datagram is missing, the
       receiving TCP will not sent an acknowledgment but will buffer all 34
       of the out-of-sequence datagrams.  After 1.5 X 2500 msec, or 3750
       msec, have elapsed the datagram times out and is resent.  It arrives
       and is acked, along with the other 34, 2500 msec later.  Before the
       lost datagram we might have been sending at the average rate a 56
       kb/s line could accept, about one every 75 msec.  After loss of the
       datagram we send at the rate of one in 6250 msec over 83 times
       slower.

       If the lost datagram in the above example is other than the first
       datagram the situation becomes the same when all of the datagrams
       before the lost datagram are acknowledged.  The example holds true
       then for any single lost datagram in the window.

       When SQ doesn't always cause datagram loss the sender continues to
       send too fast (queue size oscillates a lot).  It is important for the
       SQ to cause feed-back into the sending system as soon as possible,
       therefore when the source host IP receives an SQ it must make
       adjustments to the send rate for the datagrams still on the send
       queue not just datagrams IP is requested to send after the SQ.

       Through network delay goes up as the network queue lengths go up.

       Window size affect the chance of getting SQed.  Look at our model
       above using a queue level of 15 for node 2 before SQs are generated

    Prue & Postel                                                   [Page 9]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       and a window size of 20 datagrams.  We assumed that we could send
       data over the LAN at a sustained average rate of 1 Mb/s or about 18
       times as fast as over the WAN.  When TCP sends a burst of 20
       datagrams to node 1 they make it to node 2 in 81 msec.  The
       transition time from node 2 to node 3 is 73 msec, therefore, in 81
       msec, only one datagram is forwarded to node 3.  Thus the 17th, 18th,
       19th, and 20th datagram are lost every time we send a whole window.
       More are lost when the queue is not empty.  If a sequence of acks
       come back in response to the sent data, the acks tend to return at
       the rate at which data can traverse the net thus pacing new send data
       by opening the window at the rate which the network can accept it.
       However as soon as one datagram is lost all of the subsequent acks
       are deferred and batched until receipt of the missing data block
       which acks all of the datagrams and opens the window to 20 again.
       This causes the max queue size to be exceeded again.

       If we assume a window smaller than the max queue size in the
       bottleneck node, any time we send a window's worth of data, it is
       done independently of the current size of the queue.  The larger the
       send window, the larger a percentage of the stressed queue we send.
       If we send 50% of the stressed queue size any time that queue is more
       than 50% we threaten to overflow the queue.  Evenly spaced single
       datagram bursts have the least chance of overflowing the queue since
       they represent the minimum percentage of the max queue one may send.

       When a big window opens up (that is, a missing datagram at the head
       of a 40 datagram send queue gets retransmitted and acked), the
       perceived round trip time for datagrams subsequently sent hits a
       minimum value then goes up linearly.  The SRTT goes down then back up
       in a nice smooth curve.  This is caused by the fact IP will not add
       delay if the queue is empty and IP has not sent any datagrams to the
       destination for our introduced delay time.  But as many datagrams are
       added to the IP pre-staged send queue in bursts all have the same
       send time as far as TCP is concerned.  IP will delay each datagram on
       the head of the queue by the introduced delay amount.  The first may
       be undelayed as just described but all of the others are delayed by
       their ordinal number on the queue times the introduced delay amount.

       It seems as though in a race between a TCP session which delays
       sending to IP and one who does not, the delayer will get better
       throughput because less datagrams are lost.  The send window may also
       be increased to keep the pipeline full.  If however the non delayer
       uses windowing to reduce the chance of SQ datagram loss his
       throughput may possibly be better because no fair queuing algorithm
       is in place.

       If gateways send SQs early and don't toss data until its critical and
       keep sending SQs until a low water mark is hit, effective throughput

    Prue & Postel                                                  [Page 10]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       seems to go up.

       At the startup of our tests throughput was very high, then dropped
       off quickly as the last of the window got clobbered.  Our model
       should have used a slow start up algorithm to minimize the startup
       shock.  However the learning curve to estimate the proper value for D
       was probably quicker.

       A large part of the perceived RTT is due to the delay getting off the
       TCP2IP (TCP transitional) queue when we used large windows.  If IP
       would invoke some back-pressure to TCP in a real implementation this
       can be significantly reduced.  Reducing the window would do this for
       us at the expense of throughput.

       After an SQ burst which tosses datagrams the sender gets in a mode
       where TCP may only send one or two datagrams per RTT until the queued
       but not acked segments fall into sequence and are acked.  This
       assumes only the head of the retransmission queue is retransmitted on
       a timeout.  We can send one datagram upon timeout.  When the ack for
       the retransmission is received the window opens allowing sending a
       second.  We then wait for the next lost datagram to time out.

       If we stop sending data for a while but allow D to be decreased, our
       algorithm causes the introduced delay to dwindle away.  We would thus
       go through a new startup learning curve and network oscillation
       sequence.

       One thing not observed often was TCP timing out a segment before the
       source IP even sent the datagram the first time.  As discussed above
       the first datagram on the queue of a large burst is delayed minimally
       and succeeding datagrams have linearly increasing delays.  The
       smoothed round trip delay algorithm has a chance to adapt to the
       perceived increasing round trip times.

    Unstructured Thoughts and Comments

       The further down a route a datagram traverses before being clobbered
       the greater the waste of network resources.  SQs which do not destroy
       the datagram referred to are better than ones that do if return path
       resources are available.

       Any fix must be implementable piecemeal.  A fix can not be installed
       in all or most nodes at one time.  The SQuID algorithm fulfills this
       requirement.  It could be implemented, installed in one location, and
       used effectively.

       If it can be shown that by using the new algorithm effective
       throughput can be increased over implementations which do not

    Prue & Postel                                                  [Page 11]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       implement it that may well be effective impetus to get vendors to
       implement it.

       Once a source host has an established average minimum inter-datagram
       delay to a destination (see Appendix A), this information should be
       stored across system restarts.  This value might be used each time
       data is sent to the given host as a minimum inter-datagram delay
       value.

       Window closing algorithms reduce the average inter-datagram delay and
       the burst size but do not affect the minimum inter-datagram spacing
       by TCP.

       Currently an IP gateway node can know if it is in a critical path
       because its queues stay high or keep building up.  Its optimum queue
       size is one because it always has something to do and the through
       node delay is at a minimum.  It is very important that the gateway at
       the critical path not so discourage data flow that its queue size
       drops to zero.  If the gateway tosses datagrams this stops data flow
       for TCP for a while (as described in Observed Results above).  This
       argues for the gateway algorithm described above which SQs but does
       not toss datagrams unless necessary.  Optimally we should try to have
       a queue size somewhat larger than 1 but less than say 50% of the max
       queue size.  Large queues lead to large delay.

       TCP's SRTT is made artificially large by introducing delay at IP but
       the perceived round trip time variance is probably smaller allowing a
       smaller Beta value for the timeout value.

       So that a decrease timer is not needed for the "D" decrease function,
       upon the next sent datagram to a delayed destination just decrease
       the delay by the amount of time since we last did this divided by the
       decrease timer interval.  An alternate algorithm would be to decrease
       it by only one decrease unit amount if more than the timer interval
       has gone by.  This eliminates the problem caused by the delay, "D",
       dwindling away if we stop sending for a while.  The longer we send
       using this "D", the more likely it is that it is too large a delay
       and the more we should decrease it.

       It is better for the network and the sender for our introduced delay
       to be a little on the high side.  It minimizes the chances of getting
       a datagram clobbered by sending it into a congested gateway.  A lost
       datagram scenario described above showed that one lost datagram can
       reduce our effective delay by one to two orders of magnitude
       temporarily.  Also if the delay is a little high, the net is less
       stressed and the queues get smaller, reducing through network delay.

       The RTT experienced at a given time verses the minimum RTT possible

    Prue & Postel                                                  [Page 12]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       for the given route does give a good measure of congestion.  If we
       ever get congestion control working RTT may have little to do with
       the amount of congestion.  Effective throughput when compared with
       the possible throughput (or some other measure) is the only real
       measure of congestion.

       Slow startup of TCP is a good thing and should be encouraged as an
       additional mechanism for alleviating network overload.

       The network dynamics tends to bunch datagrams.  If we properly space
       data instead of bunching it like windowing techniques to control
       overflow of queues then greater throughput is accomplished because
       the absolute rate we can send is pacing our sending not the RTT.  We
       eliminate "stochastic bunching" [6].

       The longer the RTT the more network resources the data takes to
       traverse the net.

       Should "fair queuing" say that a longer route data transfer should
       get less band width than a shorter one (since it consumes more of the
       net)?  Being fair locally on each node may be unfair overall to
       datagrams traversing many nodes.

       If we solve congestion problems today, we will start loading up the
       net with more data tomorrow.  When this causes congestion in a year
       will that type of congestion be harder to solve than todays or is it
       not our problem?  John Nagle suggests "In a large net, we may well
       try to force congestion out to the fringes and keep the interior of
       the net uncongested by controlling entry to the net.  The IMP-based
       systems work that way, or at least used to.  This has the effect of
       concentrating congestion at the entrance to the long-haul system.
       That's where we want it; the Source Quench / congestion window / fair
       queuing set of strategies are able to handle congestion at the LAN to
       WAN bottleneck [7].  Our algorithm should try to push the network
       congestion out to the extremities and keep the interior network
       congestion free.

       Use of the algorithm is aesthetically appealing because the data is
       sitting in our local queue instead of consuming resources inside the
       net.  We give data to the network only when it is ready to accept it.

       An averaged minimum inter-datagram arrival value will give a measure
       of the network bottleneck speed at the receiver.  If the receiver
       does not defer or batch together acks the same would be learned from
       the inter-datagram arrival time of the acks.  A problem is that IP
       doesn't have knowledge of the datagram contents.  However IP does
       know from which host a datagram comes.

    Prue & Postel                                                  [Page 13]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       If SQuID limits the size of its pre-net buffering properly (causes
       back-pressure to TCP) then artificially high RTT measurements would
       not occur.

       TCP might, in the future, get a way to query IP for the current
       introduced delay, D, for a given destination and if the value is too
       excessive abort or not start a session.

       With the new algorithm TCP could have an arbitrarily large window to
       send into without fear of over running queue sizes in intermediate
       nodes (not that any TCP ever considered having this fear before).
       Thus it could have a window size which would allow it to always be
       sending; keeping the pipe full and seldom getting in the stop-and-
       wait mode of sending.  This presupposes that the local IP is able to
       cause some sort of back pressure so that the local IPs queues are not
       over run.  TCP would still be operating in the burst mode of sending
       but the local IP would be sending a datagram for the TCP as often as
       the network could accept it keeping the data flow continuous though
       potentially slow.

       Experience implementing protocols suggests avoiding timers in
       protocols whenever possible.  IP, as currently defined, does not use
       timers. The SQuID algorithm uses two at the IP level.  A way to
       eliminate the introduced delay decrease timer is to decrease the D
       value when we check the send queue for data to send.  We would
       decrease "D" by one "J" unit if "S" time, or more, has elapsed.  The
       other timer is not so easily eliminated.  If the IP implementation is
       periodically awakened to check for work to do, it could check the
       time stamps of the head of the queues to see if any datagrams have
       waited long enough.  This would mean we would necessarily wait too
       long before sending, but it may not be too large of a variance from
       our desired rates.  The additional delay would help congestion and
       reduce our chances of SQ.  Another option is setting a real timer
       which is say 25-50% too large and hope that our periodic work in IP
       will allow us to notice a datagram is delayed enough, and send it.
       Upon sending the datagram we would cancel the timer, avoiding the
       timer interrupt and environment swap.  In other implementations the
       communications interface or the link level protocol may be able to
       provide the timing needed without interrupts to the main processor.

       Background tasks like some file transfers could query IP for the
       latest delay characteristics for a given destination to determine if
       it is appropriate to consume network resources now or if it would be
       better to wait until later.

       We should consider what would happen if IP, using the SQuID
       algorithm, and TCP both introduced delay between the datagrams.  If
       TCPs delay was greater than IP's, then when IP got the datagrams it

    Prue & Postel                                                  [Page 14]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       would forward them immediately as described in the algorithm above.
       This is because when the IP send queue is empty and it has been at
       least as long as IP wants the higher level protocol, TCP, gets one
       free (no delay) send.  Note also that IP will be decreasing the
       amount of delay it wants introduced because of the successful
       transmissions without SQs.  This would affect other protocols who
       might also send to the same destination.  If TCP sends too quickly
       then IP will protect the network from its indiscretion as described
       in the basic algorithm however TCPs round trip time estimates will be
       much closer to reality.  A lost datagram will thus be detected more
       quickly.  If TCP also uses windowing to limit its sending rate, it
       might, because of its success with a smaller window, increase the
       window size increasing TCPs efficiency.

       As this algorithm is implemented everywhere, the SQ Keep (SQK) and SQ
       Low Water (SQLW) queue level percentages should be dropped to reduce
       queue sizes and thus the through net delay.  The percentage we lower
       SQK and SQLW to should be adjusted based upon the percentage of time
       the queue is empty.  The more the queue is empty the more likely it
       is that the node is discouraging data flow too much.  The more time
       the queue is not empty but not too full, the more likely it is the
       node is not excessively discouraging data flow.  How uniform the
       queue size is, is a measure of how well the network citizens are
       behaved.

       As the congestion is pushed to the sources, gateways which are
       bottlenecks can more easily detect someone not playing by the rules
       (sending datagrams in bursts) and deal with the offender.

    Prue & Postel                                                  [Page 15]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

    Appendix A -- Determination of the Value for the Parameter "I"

       To get to the correct value for the delay needed quickly, when an
       event occurred and the currently used delay was minimal, the
       transmission time for an average sized datagram across the slowest
       communications link was used for a first value.  How a real IP node
       is to guess this value is discussed below.  In our example the
       transition between node 2 and node 3 is the bottleneck. Using the 56
       kb/s line, a 512 byte datagram would take 73 msec with no queuing or
       processing time is considered.  This value is defined to be the
       minimum inter-datagram arrival time (MIAT).  Assuming a perfect
       network, ignoring factors other than transmission speed, this is the
       minimum time one could expect between receipt of datagrams at the
       destination, because of the slowed data rate through the bottleneck.
       This won't hold true if the datagrams do not follow the same path.

       The MIAT, minimum inter-datagram arrival time, may be guessed at by
       comparing the arrival timestamps of consecutive datagrams from a
       source of data.  Each value to be considered needs to be adjusted up
       or down based upon the size between the second datagram received and
       the typical datagram size.  More simply stated, a datagram which is
       half the size of the average datagram can be transmitted across a
       line in half the time.  Therefore, double its IAT before considering
       it for an MIAT.  If the timestamp of a datagrams is taken based upon
       an event caused by the start of the datagram arriving, not the
       completion of the datagram arriving, then the first datagram's size
       is the limiting length and should be used to adjust its IAT.  In
       order to keep the algorithm simple, arrival times for short datagram
       could be ignored as could IATs which were orders of magnitude too
       large (see below).

       Once a minimal value is found based upon looking for small values
       over a minute or more, the value might be time averaged with a value
       kept like TCP's SRTT in order to reduce the effects of a false MIAT.
       We could assume the limiting facility would be a 9.6 kb/s line, a
       56-64 kb/s line, or a 1.5 Mb/s line.  These facilities would provide
       a MIAT of 427 msec, 73-64 msec, or 3 msec respectively, for a
       datagram 512 bytes long.  These are almost orders of magnitude in
       differences.  If the MIAT a node measures is not in this range but
       close, the value it is closest to may be used for its MIAT from that
       source.

       One of the good things about this measurement is that it is an
       entirely passive measurement.  No additional traffic is needed to
       measure it.  If a source is not sending data continuously then the
       longer measured values won't be validated as minimal values.  The
       assumption is that at least sometimes the source will send multiple
       datagrams at a time.

    Prue & Postel                                                  [Page 16]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

       The MIAT measurement is totally unaffected by satellite delay
       characteristics of any intervening facilities.  The chance of getting
       a valid minimal reading is affected by the number of nodes traversed,
       but the value measured if it is valid will not be affected by the
       number of nodes traversed.  Stated another way, when a pair of
       datagrams traverse from one node to the next the datagrams are
       susceptible to being separated by a datagram from another source.
       Both of these factors affect SRTT. The value obtained requires no
       topological knowledge of the route.

       A potential problem with the measurement is, it will not be the
       proper value for some forms of alternate routes.  If a T1 link is the
       bottleneck route some times and other times it is a 56 kb/s link our
       first guess for inter-datagram delay would be too small for the 56
       kb/s line route.  Another problem is that if one datagram goes via
       one route and the next goes via another, their inter-datagram arrival
       difference could lead to a small false measurement.  If intervening
       networks fragment datagrams then the measured IAT between segments
       could be misleading.  A solution to this problem is to ignore
       fragmented datagram IATs.

       This number represents the minimum inter-datagram delay the sending
       IP should use to send to us, the measuring site, for the given
       datagram size.  If we assume that the return path will be through the
       same facilities or the same type, then as described above this value
       can be the first guess for inter-datagram introduced delay, "D" (in
       the algorithm).  It represents the "I" parameter.

       These MIATs may be cached on a host, subnet, or network basis.  The
       last "n" hosts MIATs could be kept.  For infrequent destinations an
       entry per destination network would be applicable to many
       destinations.  If the local net is in fact a subnet, then the other
       local subnet MIATs could be kept.

       If a good algorithm is found for MIAT, comparing it to the average
       IAT (during data transfer) would give a good measure of the amount of
       network traffic load.  Since IP has no idea when the source of data
       is sending as fast as possible, to get a valid average, upper layer
       protocols would have to figure this out for themselves.  IP could
       however provide an interface to get the current MIAT for a given
       destination.

    Prue & Postel                                                  [Page 17]

    RFC 1016        Source Quench Introduced Delay -- SQuID        July 1987

    References

       [1]  Postel, Jon, "Internet Protocol - DARPA Internet Program
       Protocol Specification", RFC 791, ISI, September 1981.

       [2]  Postel, Jon, "Internet Control Message Protocol - DARPA Internet
       Program Protocol Specification", RFC 792, ISI, September 1981.

       [3]  Karels, M., "Re: Source Quench", electronic mail message to J.
       Postel and INENG-INTEREST, Tue, 24 Feb 87.

       [4] Nagle, John B., "On Packet Switches With Infinite Storage", RFC
       970, FACC Palo Alto, December 1985.

       [5] Jacobson, Van, "Re: interpacket arrival variance and mean",
       electronic mail message to TCP-IP,  Mon, 15 Jun 87 06:08:01 PDT

       [6] Jacobson, Van, "Re: Appropriate measures of gateway performance"
       electronic mail message to J. Noel Chiappa  and INENG-INTEREST, Sun,
       22 Mar 87 15:04:44 PST.

       [7] Nagle, John B., "Source quench, and congestion generally",
       electronic mail message to B. Braden and INENG-INTEREST, Thu, 5 Mar
       87 11:08:49 PST.

       [8] Nagle, John B., "Congestion Control in IP/TCP Internetworks", RFC
       896, FACC Palo Alto, 6 January 1984.

    Prue & Postel                                                  [Page 18]