    Internet Engineering Task Force (IETF)                        P. Hoffman
    Request for Comments: 7719                                         ICANN
    Category: Informational                                      A. Sullivan
    ISSN: 2070-1721                                                      Dyn
                                                                 K. Fujiwara
                                                                        JPRS
                                                               December 2015

                                DNS Terminology

    Abstract

       The DNS is defined in literally dozens of different RFCs.  The
       terminology used by implementers and developers of DNS protocols, and
       by operators of DNS systems, has sometimes changed in the decades
       since the DNS was first defined.  This document gives current
       definitions for many of the terms used in the DNS in a single
       document.

    Status of This Memo

       This document is not an Internet Standards Track specification; it is
       published for informational purposes.

       This document is a product of the Internet Engineering Task Force
       (IETF).  It represents the consensus of the IETF community.  It has
       received public review and has been approved for publication by the
       Internet Engineering Steering Group (IESG).  Not all documents
       approved by the IESG are a candidate for any level of Internet
       Standard; see Section 2 of RFC 5741.

       Information about the current status of this document, any errata,
       and how to provide feedback on it may be obtained at
       http://www.rfc-editor.org/info/rfc7719.

    Hoffman, et al.               Informational                     [Page 1]

    RFC 7719                     DNS Terminology               December 2015

    Copyright Notice

       Copyright (c) 2015 IETF Trust and the persons identified as the
       document authors.  All rights reserved.

       This document is subject to BCP 78 and the IETF Trust's Legal
       Provisions Relating to IETF Documents
       (http://trustee.ietf.org/license-info) in effect on the date of
       publication of this document.  Please review these documents
       carefully, as they describe your rights and restrictions with respect
       to this document.  Code Components extracted from this document must
       include Simplified BSD License text as described in Section 4.e of
       the Trust Legal Provisions and are provided without warranty as
       described in the Simplified BSD License.

    Table of Contents

       1.  Introduction  . . . . . . . . . . . . . . . . . . . . . . . .   2
       2.  Names . . . . . . . . . . . . . . . . . . . . . . . . . . . .   4
       3.  DNS Header and Response Codes . . . . . . . . . . . . . . . .   6
       4.  Resource Records  . . . . . . . . . . . . . . . . . . . . . .   7
       5.  DNS Servers and Clients . . . . . . . . . . . . . . . . . . .   9
       6.  Zones . . . . . . . . . . . . . . . . . . . . . . . . . . . .  13
       7.  Registration Model  . . . . . . . . . . . . . . . . . . . . .  17
       8.  General DNSSEC  . . . . . . . . . . . . . . . . . . . . . . .  18
       9.  DNSSEC States . . . . . . . . . . . . . . . . . . . . . . . .  20
       10. Security Considerations . . . . . . . . . . . . . . . . . . .  22
       11. References  . . . . . . . . . . . . . . . . . . . . . . . . .  22
         11.1.  Normative References . . . . . . . . . . . . . . . . . .  22
         11.2.  Informative References . . . . . . . . . . . . . . . . .  24
       Acknowledgements  . . . . . . . . . . . . . . . . . . . . . . . .  27
       Authors' Addresses  . . . . . . . . . . . . . . . . . . . . . . .  27

    1.  Introduction

       The Domain Name System (DNS) is a simple query-response protocol
       whose messages in both directions have the same format.  The protocol
       and message format are defined in [RFC1034] and [RFC1035].  These
       RFCs defined some terms, but later documents defined others.  Some of
       the terms from RFCs 1034 and 1035 now have somewhat different
       meanings than they did in 1987.

       This document collects a wide variety of DNS-related terms.  Some of
       them have been precisely defined in earlier RFCs, some have been
       loosely defined in earlier RFCs, and some are not defined in any
       earlier RFC at all.

    Hoffman, et al.               Informational                     [Page 2]

    RFC 7719                     DNS Terminology               December 2015

       Most of the definitions here are the consensus definition of the DNS
       community -- both protocol developers and operators.  Some of the
       definitions differ from earlier RFCs, and those differences are
       noted.  In this document, where the consensus definition is the same
       as the one in an RFC, that RFC is quoted.  Where the consensus
       definition has changed somewhat, the RFC is mentioned but the new
       stand-alone definition is given.

       It is important to note that, during the development of this
       document, it became clear that some DNS-related terms are interpreted
       quite differently by different DNS experts.  Further, some terms that
       are defined in early DNS RFCs now have definitions that are generally
       agreed to, but that are different from the original definitions.
       Therefore, the authors intend to follow this document with a
       substantial revision in the not-distant future.  That revision will
       probably have more in-depth discussion of some terms as well as new
       terms; it will also update some of the RFCs with new definitions.

       The terms are organized loosely by topic.  Some definitions are for
       new terms for things that are commonly talked about in the DNS
       community but that never had terms defined for them.

       Other organizations sometimes define DNS-related terms their own way.
       For example, the W3C defines "domain" at
       https://specs.webplatform.org/url/webspecs/develop/.

       Note that there is no single consistent definition of "the DNS".  It
       can be considered to be some combination of the following: a commonly
       used naming scheme for objects on the Internet; a distributed
       database representing the names and certain properties of these
       objects; an architecture providing distributed maintenance,
       resilience, and loose coherency for this database; and a simple
       query-response protocol (as mentioned below) implementing this
       architecture.

       Capitalization in DNS terms is often inconsistent among RFCs and
       various DNS practitioners.  The capitalization used in this document
       is a best guess at current practices, and is not meant to indicate
       that other capitalization styles are wrong or archaic.  In some
       cases, multiple styles of capitalization are used for the same term
       due to quoting from different RFCs.

    Hoffman, et al.               Informational                     [Page 3]

    RFC 7719                     DNS Terminology               December 2015

    2.  Names

       Domain name:  Section 3.1 of [RFC1034] talks of "the domain name
          space" as a tree structure.  "Each node has a label, which is zero
          to 63 octets in length. ... The domain name of a node is the list
          of the labels on the path from the node to the root of the tree.
          ... To simplify implementations, the total number of octets that
          represent a domain name (i.e., the sum of all label octets and
          label lengths) is limited to 255."  Any label in a domain name can
          contain any octet value.

       Fully qualified domain name (FQDN):  This is often just a clear way
          of saying the same thing as "domain name of a node", as outlined
          above.  However, the term is ambiguous.  Strictly speaking, a
          fully qualified domain name would include every label, including
          the final, zero-length label of the root: such a name would be
          written "www.example.net." (note the terminating dot).  But
          because every name eventually shares the common root, names are
          often written relative to the root (such as "www.example.net") and
          are still called "fully qualified".  This term first appeared in
          [RFC819].  In this document, names are often written relative to
          the root.

          The need for the term "fully qualified domain name" comes from the
          existence of partially qualified domain names, which are names
          where some of the right-most names are left off and are understood
          only by context.

       Label:  The identifier of an individual node in the sequence of nodes
          identified by a fully qualified domain name.

       Host name:  This term and its equivalent, "hostname", have been
          widely used but are not defined in [RFC1034], [RFC1035],
          [RFC1123], or [RFC2181].  The DNS was originally deployed into the
          Host Tables environment as outlined in [RFC952], and it is likely
          that the term followed informally from the definition there.  Over
          time, the definition seems to have shifted.  "Host name" is often
          meant to be a domain name that follows the rules in Section 3.5 of
          [RFC1034], the "preferred name syntax".  Note that any label in a
          domain name can contain any octet value; hostnames are generally
          considered to be domain names where every label follows the rules
          in the "preferred name syntax", with the amendment that labels can
          start with ASCII digits (this amendment comes from Section 2.1 of
          [RFC1123]).

          People also sometimes use the term hostname to refer to just the
          first label of an FQDN, such as "printer" in
          "printer.admin.example.com".  (Sometimes this is formalized in

    Hoffman, et al.               Informational                     [Page 4]

    RFC 7719                     DNS Terminology               December 2015

          configuration in operating systems.)  In addition, people
          sometimes use this term to describe any name that refers to a
          machine, and those might include labels that do not conform to the
          "preferred name syntax".

       TLD:  A Top-Level Domain, meaning a zone that is one layer below the
          root, such as "com" or "jp".  There is nothing special, from the
          point of view of the DNS, about TLDs.  Most of them are also
          delegation-centric zones, and there are significant policy issues
          around their operation.  TLDs are often divided into sub-groups
          such as Country Code Top-Level Domains (ccTLDs), Generic Top-Level
          Domains (gTLDs), and others; the division is a matter of policy,
          and beyond the scope of this document.

       IDN:  The common abbreviation for "Internationalized Domain Name".
          The IDNA protocol is the standard mechanism for handling domain
          names with non-ASCII characters in applications in the DNS.  The
          current standard, normally called "IDNA2008", is defined in
          [RFC5890], [RFC5891], [RFC5892], [RFC5893], and [RFC5894].  These
          documents define many IDN-specific terms such as "LDH label",
          "A-label", and "U-label".  [RFC6365] defines more terms that
          relate to internationalization (some of which relate to IDNs), and
          [RFC6055] has a much more extensive discussion of IDNs, including
          some new terminology.

       Subdomain:  "A domain is a subdomain of another domain if it is
          contained within that domain.  This relationship can be tested by
          seeing if the subdomain's name ends with the containing domain's
          name."  (Quoted from [RFC1034], Section 3.1).  For example, in the
          host name "nnn.mmm.example.com", both "mmm.example.com" and
          "nnn.mmm.example.com" are subdomains of "example.com".

       Alias:  The owner of a CNAME resource record, or a subdomain of the
          owner of a DNAME resource record [RFC6672].  See also "canonical
          name".

       Canonical name:  A CNAME resource record "identifies its owner name
          as an alias, and specifies the corresponding canonical name in the
          RDATA section of the RR."  (Quoted from [RFC1034], Section 3.6.2)
          This usage of the word "canonical" is related to the mathematical
          concept of "canonical form".

       CNAME:  "It is traditional to refer to the owner of a CNAME record as
          'a CNAME'.  This is unfortunate, as 'CNAME' is an abbreviation of
          'canonical name', and the owner of a CNAME record is an alias, not
          a canonical name."  (Quoted from [RFC2181], Section 10.1.1)

    Hoffman, et al.               Informational                     [Page 5]

    RFC 7719                     DNS Terminology               December 2015

       Public suffix:  "A domain that is controlled by a public registry."
          (Quoted from [RFC6265], Section 5.3) A common definition for this
          term is a domain under which subdomains can be registered, and on
          which HTTP cookies ([RFC6265]) should not be set.  There is no
          indication in a domain name whether it is a public suffix; that
          can only be determined by outside means.  In fact, both a domain
          and a subdomain of that domain can be public suffixes.  At the
          time this document is published, the IETF DBOUND Working Group
          [DBOUND] is dealing with issues concerning public suffixes.

          There is nothing inherent in a domain name to indicate whether it
          is a public suffix.  One resource for identifying public suffixes
          is the Public Suffix List (PSL) maintained by Mozilla
          (http://publicsuffix.org/).

          For example, at the time this document is published, the "com.au"
          domain is listed as a public suffix in the PSL.  (Note that this
          example might change in the future.)

          Note that the term "public suffix" is controversial in the DNS
          community for many reasons, and may be significantly changed in
          the future.  One example of the difficulty of calling a domain a
          public suffix is that designation can change over time as the
          registration policy for the zone changes, such as the case of the
          "uk" TLD around the time this document is published.

    3.  DNS Header and Response Codes

       The header of a DNS message is its first 12 octets.  Many of the
       fields and flags in the header diagram in Sections 4.1.1 through
       4.1.3 of [RFC1035] are referred to by their names in that diagram.
       For example, the response codes are called "RCODEs", the data for a
       record is called the "RDATA", and the authoritative answer bit is
       often called "the AA flag" or "the AA bit".

       Some of response codes that are defined in [RFC1035] have gotten
       their own shorthand names.  Some common response code names that
       appear without reference to the numeric value are "FORMERR",
       "SERVFAIL", and "NXDOMAIN" (the latter of which is also referred to
       as "Name Error").  All of the RCODEs are listed at
       http://www.iana.org/assignments/dns-parameters, although that site
       uses mixed-case capitalization, while most documents use all-caps.

       NODATA:  "A pseudo RCODE which indicates that the name is valid for
          the given class, but there are no records of the given type.  A
          NODATA response has to be inferred from the answer."  (Quoted from
          [RFC2308], Section 1.)  "NODATA is indicated by an answer with the
          RCODE set to NOERROR and no relevant answers in the answer

    Hoffman, et al.               Informational                     [Page 6]

    RFC 7719                     DNS Terminology               December 2015

          section.  The authority section will contain an SOA record, or
          there will be no NS records there."  (Quoted from [RFC2308],
          Section 2.2.)  Note that referrals have a similar format to NODATA
          replies; [RFC2308] explains how to distinguish them.

          The term "NXRRSET" is sometimes used as a synonym for NODATA.
          However, this is a mistake, given that NXRRSET is a specific error
          code defined in [RFC2136].

       Negative response:  A response that indicates that a particular RRset
          does not exist, or whose RCODE indicates the nameserver cannot
          answer.  Sections 2 and 7 of [RFC2308] describe the types of
          negative responses in detail.

       Referrals:  Data from the authority section of a non-authoritative
          answer.  [RFC1035] Section 2.1 defines "authoritative" data.
          However, referrals at zone cuts (defined in Section 6) are not
          authoritative.  Referrals may be zone cut NS resource records and
          their glue records.  NS records on the parent side of a zone cut
          are an authoritative delegation, but are normally not treated as
          authoritative data.  In general, a referral is a way for a server
          to send an answer saying that the server does not know the answer,
          but knows where the query should be directed in order to get an
          answer.  Historically, many authoritative servers answered with a
          referral to the root zone when queried for a name for which they
          were not authoritative, but this practice has declined.

    4.  Resource Records

       RR:  An acronym for resource record.  ([RFC1034], Section 3.6.)

       RRset:  A set of resource records with the same label, class and
          type, but with different data.  (Definition from [RFC2181]) Also
          spelled RRSet in some documents.  As a clarification, "same label"
          in this definition means "same owner name".  In addition,
          [RFC2181] states that "the TTLs of all RRs in an RRSet must be the
          same".  (This definition is definitely not the same as "the
          response one gets to a query for QTYPE=ANY", which is an
          unfortunate misunderstanding.)

       EDNS:  The extension mechanisms for DNS, defined in [RFC6891].
          Sometimes called "EDNS0" or "EDNS(0)" to indicate the version
          number.  EDNS allows DNS clients and servers to specify message
          sizes larger than the original 512 octet limit, to expand the
          response code space, and potentially to carry additional options
          that affect the handling of a DNS query.

    Hoffman, et al.               Informational                     [Page 7]

    RFC 7719                     DNS Terminology               December 2015

       OPT:  A pseudo-RR (sometimes called a "meta-RR") that is used only to
          contain control information pertaining to the question-and-answer
          sequence of a specific transaction.  (Definition from [RFC6891],
          Section 6.1.1) It is used by EDNS.

       Owner:  The domain name where a RR is found ([RFC1034], Section 3.6).
          Often appears in the term "owner name".

       SOA field names:  DNS documents, including the definitions here,
          often refer to the fields in the RDATA of an SOA resource record
          by field name.  Those fields are defined in Section 3.3.13 of
          [RFC1035].  The names (in the order they appear in the SOA RDATA)
          are MNAME, RNAME, SERIAL, REFRESH, RETRY, EXPIRE, and MINIMUM.
          Note that the meaning of MINIMUM field is updated in Section 4 of
          [RFC2308]; the new definition is that the MINIMUM field is only
          "the TTL to be used for negative responses".  This document tends
          to use field names instead of terms that describe the fields.

       TTL:  The maximum "time to live" of a resource record.  "A TTL value
          is an unsigned number, with a minimum value of 0, and a maximum
          value of 2147483647.  That is, a maximum of 2^31 - 1.  When
          transmitted, the TTL is encoded in the less significant 31 bits of
          the 32 bit TTL field, with the most significant, or sign, bit set
          to zero."  (Quoted from [RFC2181], Section 8) (Note that [RFC1035]
          erroneously stated that this is a signed integer; that was fixed
          by [RFC2181].)

          The TTL "specifies the time interval that the resource record may
          be cached before the source of the information should again be
          consulted".  (Quoted from [RFC1035], Section 3.2.1) Also: "the
          time interval (in seconds) that the resource record may be cached
          before it should be discarded".  (Quoted from [RFC1035],
          Section 4.1.3).  Despite being defined for a resource record, the
          TTL of every resource record in an RRset is required to be the
          same ([RFC2181], Section 5.2).

          The reason that the TTL is the maximum time to live is that a
          cache operator might decide to shorten the time to live for
          operational purposes, such as if there is a policy to disallow TTL
          values over a certain number.  Also, if a value is flushed from
          the cache when its value is still positive, the value effectively
          becomes zero.  Some servers are known to ignore the TTL on some
          RRsets (such as when the authoritative data has a very short TTL)
          even though this is against the advice in RFC 1035.

    Hoffman, et al.               Informational                     [Page 8]

    RFC 7719                     DNS Terminology               December 2015

          There is also the concept of a "default TTL" for a zone, which can
          be a configuration parameter in the server software.  This is
          often expressed by a default for the entire server, and a default
          for a zone using the $TTL directive in a zone file.  The $TTL
          directive was added to the master file format by [RFC2308].

       Class independent:  A resource record type whose syntax and semantics
          are the same for every DNS class.  A resource record type that is
          not class independent has different meanings depending on the DNS
          class of the record, or the meaning is undefined for classes other
          than IN (class 1, the Internet).

    5.  DNS Servers and Clients

       This section defines the terms used for the systems that act as DNS
       clients, DNS servers, or both.

       Resolver:  A program "that extract[s] information from name servers
          in response to client requests."  (Quoted from [RFC1034],
          Section 2.4) "The resolver is located on the same machine as the
          program that requests the resolver's services, but it may need to
          consult name servers on other hosts."  (Quoted from [RFC1034],
          Section 5.1) A resolver performs queries for a name, type, and
          class, and receives answers.  The logical function is called
          "resolution".  In practice, the term is usually referring to some
          specific type of resolver (some of which are defined below), and
          understanding the use of the term depends on understanding the
          context.

       Stub resolver:  A resolver that cannot perform all resolution itself.
          Stub resolvers generally depend on a recursive resolver to
          undertake the actual resolution function.  Stub resolvers are
          discussed but never fully defined in Section 5.3.1 of [RFC1034].
          They are fully defined in Section 6.1.3.1 of [RFC1123].

       Iterative mode:  A resolution mode of a server that receives DNS
          queries and responds with a referral to another server.
          Section 2.3 of [RFC1034] describes this as "The server refers the
          client to another server and lets the client pursue the query".  A
          resolver that works in iterative mode is sometimes called an
          "iterative resolver".

       Recursive mode:  A resolution mode of a server that receives DNS
          queries and either responds to those queries from a local cache or
          sends queries to other servers in order to get the final answers
          to the original queries.  Section 2.3 of [RFC1034] describes this
          as "The first server pursues the query for the client at another
          server".  A server operating in recursive mode may be thought of

    Hoffman, et al.               Informational                     [Page 9]

    RFC 7719                     DNS Terminology               December 2015

          as having a name server side (which is what answers the query) and
          a resolver side (which performs the resolution function).  Systems
          operating in this mode are commonly called "recursive servers".
          Sometimes they are called "recursive resolvers".  While strictly
          the difference between these is that one of them sends queries to
          another recursive server and the other does not, in practice it is
          not possible to know in advance whether the server that one is
          querying will also perform recursion; both terms can be observed
          in use interchangeably.

       Full resolver:  This term is used in [RFC1035], but it is not defined
          there.  RFC 1123 defines a "full-service resolver" that may or may
          not be what was intended by "full resolver" in [RFC1035].  This
          term is not properly defined in any RFC.

       Full-service resolver:  Section 6.1.3.1 of [RFC1123] defines this
          term to mean a resolver that acts in recursive mode with a cache
          (and meets other requirements).

       Priming:  The mechanism used by a resolver to determine where to send
          queries before there is anything in the resolver's cache.  Priming
          is most often done from a configuration setting that contains a
          list of authoritative servers for the root zone.

       Negative caching:  "The storage of knowledge that something does not
          exist, cannot give an answer, or does not give an answer."
          (Quoted from [RFC2308], Section 1)

       Authoritative server:  "A server that knows the content of a DNS zone
          from local knowledge, and thus can answer queries about that zone
          without needing to query other servers."  (Quoted from [RFC2182],
          Section 2.)  It is a system that responds to DNS queries with
          information about zones for which it has been configured to answer
          with the AA flag in the response header set to 1.  It is a server
          that has authority over one or more DNS zones.  Note that it is
          possible for an authoritative server to respond to a query without
          the parent zone delegating authority to that server.
          Authoritative servers also provide "referrals", usually to child
          zones delegated from them; these referrals have the AA bit set to
          0 and come with referral data in the Authority and (if needed) the
          Additional sections.

       Authoritative-only server:  A name server that only serves
          authoritative data and ignores requests for recursion.  It will
          "not normally generate any queries of its own.  Instead, it
          answers non-recursive queries from iterative resolvers looking for
          information in zones it serves."  (Quoted from [RFC4697],
          Section 2.4)

    Hoffman, et al.               Informational                    [Page 10]

    RFC 7719                     DNS Terminology               December 2015

       Zone transfer:  The act of a client requesting a copy of a zone and
          an authoritative server sending the needed information.  (See
          Section 6 for a description of zones.)  There are two common
          standard ways to do zone transfers: the AXFR ("Authoritative
          Transfer") mechanism to copy the full zone (described in
          [RFC5936], and the IXFR ("Incremental Transfer") mechanism to copy
          only parts of the zone that have changed (described in [RFC1995]).
          Many systems use non-standard methods for zone transfer outside
          the DNS protocol.

       Secondary server:  "An authoritative server which uses zone transfer
          to retrieve the zone" (Quoted from [RFC1996], Section 2.1).
          [RFC2182] describes secondary servers in detail.  Although early
          DNS RFCs such as [RFC1996] referred to this as a "slave", the
          current common usage has shifted to calling it a "secondary".
          Secondary servers are also discussed in [RFC1034].

       Slave server:  See secondary server.

       Primary server:  "Any authoritative server configured to be the
          source of zone transfer for one or more [secondary] servers"
          (Quoted from [RFC1996], Section 2.1) or, more specifically, "an
          authoritative server configured to be the source of AXFR or IXFR
          data for one or more [secondary] servers" (Quoted from [RFC2136]).
          Although early DNS RFCs such as [RFC1996] referred to this as a
          "master", the current common usage has shifted to "primary".
          Primary servers are also discussed in [RFC1034].

       Master server:  See primary server.

       Primary master:  "The primary master is named in the zone's SOA MNAME
          field and optionally by an NS RR".  (Quoted from [RFC1996],
          Section 2.1).  [RFC2136] defines "primary master" as "Master
          server at the root of the AXFR/IXFR dependency graph.  The primary
          master is named in the zone's SOA MNAME field and optionally by an
          NS RR.  There is by definition only one primary master server per
          zone."  The idea of a primary master is only used by [RFC2136],
          and is considered archaic in other parts of the DNS.

       Stealth server:  This is "like a slave server except not listed in an
          NS RR for the zone."  (Quoted from [RFC1996], Section 2.1)

    Hoffman, et al.               Informational                    [Page 11]

    RFC 7719                     DNS Terminology               December 2015

       Hidden master:  A stealth server that is a master for zone transfers.
          "In this arrangement, the master name server that processes the
          updates is unavailable to general hosts on the Internet; it is not
          listed in the NS RRset."  (Quoted from [RFC6781], Section 3.4.3.)
          An earlier RFC, [RFC4641], said that the hidden master's name
          appears in the SOA RRs MNAME field, although in some setups, the
          name does not appear at all in the public DNS.  A hidden master
          can be either a secondary or a primary master.

       Forwarding:  The process of one server sending a DNS query with the
          RD bit set to 1 to another server to resolve that query.
          Forwarding is a function of a DNS resolver; it is different than
          simply blindly relaying queries.

          [RFC5625] does not give a specific definition for forwarding, but
          describes in detail what features a system that forwards need to
          support.  Systems that forward are sometimes called "DNS proxies",
          but that term has not yet been defined (even in [RFC5625]).

       Forwarder:  Section 1 of [RFC2308] describes a forwarder as "a
          nameserver used to resolve queries instead of directly using the
          authoritative nameserver chain".  [RFC2308] further says "The
          forwarder typically either has better access to the internet, or
          maintains a bigger cache which may be shared amongst many
          resolvers."  That definition appears to suggest that forwarders
          normally only query authoritative servers.  In current use,
          however, forwarders often stand between stub resolvers and
          recursive servers.  [RFC2308] is silent on whether a forwarder is
          iterative-only or can be a full-service resolver.

       Policy-implementing resolver:  A resolver acting in recursive mode
          that changes some of the answers that it returns based on policy
          criteria, such as to prevent access to malware sites or
          objectionable content.  In general, a stub resolver has no idea
          whether upstream resolvers implement such policy or, if they do,
          the exact policy about what changes will be made.  In some cases,
          the user of the stub resolver has selected the policy-implementing
          resolver with the explicit intention of using it to implement the
          policies.  In other cases, policies are imposed without the user
          of the stub resolver being informed.

       Open resolver:  A full-service resolver that accepts and processes
          queries from any (or nearly any) stub resolver.  This is sometimes
          also called a "public resolver", although the term "public
          resolver" is used more with open resolvers that are meant to be
          open, as compared to the vast majority of open resolvers that are
          probably misconfigured to be open.

    Hoffman, et al.               Informational                    [Page 12]

    RFC 7719                     DNS Terminology               December 2015

       View:  A configuration for a DNS server that allows it to provide
          different answers depending on attributes of the query.
          Typically, views differ by the source IP address of a query, but
          can also be based on the destination IP address, the type of query
          (such as AXFR), whether it is recursive, and so on.  Views are
          often used to provide more names or different addresses to queries
          from "inside" a protected network than to those "outside" that
          network.  Views are not a standardized part of the DNS, but they
          are widely implemented in server software.

       Passive DNS:  A mechanism to collect large amounts of DNS data by
          storing DNS responses from servers.  Some of these systems also
          collect the DNS queries associated with the responses; this can
          raise privacy issues.  Passive DNS databases can be used to answer
          historical questions about DNS zones such as which records were
          available for them at what times in the past.  Passive DNS
          databases allow searching of the stored records on keys other than
          just the name, such as "find all names which have A records of a
          particular value".

       Anycast:  "The practice of making a particular service address
          available in multiple, discrete, autonomous locations, such that
          datagrams sent are routed to one of several available locations."
          (Quoted from [RFC4786], Section 2)

    6.  Zones

       This section defines terms that are used when discussing zones that
       are being served or retrieved.

       Zone:  "Authoritative information is organized into units called
          'zones', and these zones can be automatically distributed to the
          name servers which provide redundant service for the data in a
          zone."  (Quoted from [RFC1034], Section 2.4)

       Child:  "The entity on record that has the delegation of the domain
          from the Parent."  (Quoted from [RFC7344], Section 1.1)

       Parent:  "The domain in which the Child is registered."  (Quoted from
          [RFC7344], Section 1.1) Earlier, "parent name server" was defined
          in [RFC882] as "the name server that has authority over the place
          in the domain name space that will hold the new domain".  (Note
          that [RFC882] was obsoleted by [RFC1034] and [RFC1035].)  [RFC819]
          also has some description of the relationship between parents and
          children.

    Hoffman, et al.               Informational                    [Page 13]

    RFC 7719                     DNS Terminology               December 2015

       Origin:

          (a) "The domain name that appears at the top of a zone (just below
          the cut that separates the zone from its parent).  The name of the
          zone is the same as the name of the domain at the zone's origin."
          (Quoted from [RFC2181], Section 6.)  These days, this sense of
          "origin" and "apex" (defined below) are often used
          interchangeably.

          (b) The domain name within which a given relative domain name
          appears in zone files.  Generally seen in the context of
          "$ORIGIN", which is a control entry defined in [RFC1035],
          Section 5.1, as part of the master file format.  For example, if
          the $ORIGIN is set to "example.org.", then a master file line for
          "www" is in fact an entry for "www.example.org.".

       Apex:  The point in the tree at an owner of an SOA and corresponding
          authoritative NS RRset.  This is also called the "zone apex".
          [RFC4033] defines it as "the name at the child's side of a zone
          cut".  The "apex" can usefully be thought of as a data-theoretic
          description of a tree structure, and "origin" is the name of the
          same concept when it is implemented in zone files.  The
          distinction is not always maintained in use, however, and one can
          find uses that conflict subtly with this definition.  [RFC1034]
          uses the term "top node of the zone" as a synonym of "apex", but
          that term is not widely used.  These days, the first sense of
          "origin" (above) and "apex" are often used interchangeably.

       Zone cut:  The delimitation point between two zones where the origin
          of one of the zones is the child of the other zone.

          "Zones are delimited by 'zone cuts'.  Each zone cut separates a
          'child' zone (below the cut) from a 'parent' zone (above the cut).
          (Quoted from [RFC2181], Section 6; note that this is barely an
          ostensive definition.)  Section 4.2 of [RFC1034] uses "cuts" as
          'zone cut'."

       Delegation:  The process by which a separate zone is created in the
          name space beneath the apex of a given domain.  Delegation happens
          when an NS RRset is added in the parent zone for the child origin.
          Delegation inherently happens at a zone cut.  The term is also
          commonly a noun: the new zone that is created by the act of
          delegating.

    Hoffman, et al.               Informational                    [Page 14]

    RFC 7719                     DNS Terminology               December 2015

       Glue records:  "[Resource records] which are not part of the
          authoritative data [of the zone], and are address resource records
          for the [name servers in subzones].  These RRs are only necessary
          if the name server's name is 'below' the cut, and are only used as
          part of a referral response."  Without glue "we could be faced
          with the situation where the NS RRs tell us that in order to learn
          a name server's address, we should contact the server using the
          address we wish to learn."  (Definition from [RFC1034],
          Section 4.2.1)

          A later definition is that glue "includes any record in a zone
          file that is not properly part of that zone, including nameserver
          records of delegated sub-zones (NS records), address records that
          accompany those NS records (A, AAAA, etc), and any other stray
          data that might appear" ([RFC2181], Section 5.4.1).  Although glue
          is sometimes used today with this wider definition in mind, the
          context surrounding the [RFC2181] definition suggests it is
          intended to apply to the use of glue within the document itself
          and not necessarily beyond.

       In-bailiwick:

          (a) An adjective to describe a name server whose name is either
          subordinate to or (rarely) the same as the zone origin.  In-
          bailiwick name servers require glue records in their parent zone
          (using the first of the definitions of "glue records" in the
          definition above).

          (b) Data for which the server is either authoritative, or else
          authoritative for an ancestor of the owner name.  This sense of
          the term normally is used when discussing the relevancy of glue
          records in a response.  For example, the server for the parent
          zone "example.com" might reply with glue records for
          "ns.child.example.com".  Because the "child.example.com" zone is a
          descendant of the "example.com" zone, the glue records are in-
          bailiwick.

       Out-of-bailiwick:  The antonym of in-bailiwick.

       Authoritative data:  "All of the RRs attached to all of the nodes
          from the top node of the zone down to leaf nodes or nodes above
          cuts around the bottom edge of the zone."  (Quoted from [RFC1034],
          Section 4.2.1) It is noted that this definition might
          inadvertently also include any NS records that appear in the zone,
          even those that might not truly be authoritative because there are
          identical NS RRs below the zone cut.  This reveals the ambiguity

    Hoffman, et al.               Informational                    [Page 15]

    RFC 7719                     DNS Terminology               December 2015

          in the notion of authoritative data, because the parent-side NS
          records authoritatively indicate the delegation, even though they
          are not themselves authoritative data.

       Root zone:  The zone whose apex is the zero-length label.  Also
          sometimes called "the DNS root".

       Empty non-terminals:  "Domain names that own no resource records but
          have subdomains that do."  (Quoted from [RFC4592], Section 2.2.2.)
          A typical example is in SRV records: in the name
          "_sip._tcp.example.com", it is likely that "_tcp.example.com" has
          no RRsets, but that "_sip._tcp.example.com" has (at least) an SRV
          RRset.

       Delegation-centric zone:  A zone that consists mostly of delegations
          to child zones.  This term is used in contrast to a zone that
          might have some delegations to child zones, but also has many data
          resource records for the zone itself and/or for child zones.  The
          term is used in [RFC4956] and [RFC5155], but is not defined there.

       Wildcard:  [RFC1034] defined "wildcard", but in a way that turned out
          to be confusing to implementers.  Special treatment is given to
          RRs with owner names starting with the label "*".  "Such RRs are
          called 'wildcards'.  Wildcard RRs can be thought of as
          instructions for synthesizing RRs."  (Quoted from [RFC1034],
          Section 4.3.3) For an extended discussion of wildcards, including
          clearer definitions, see [RFC4592].

       Occluded name:  "The addition of a delegation point via dynamic
          update will render all subordinate domain names to be in a limbo,
          still part of the zone, but not available to the lookup process.
          The addition of a DNAME resource record has the same impact.  The
          subordinate names are said to be 'occluded'."  (Quoted from
          [RFC5936], Section 3.5)

       Fast flux DNS:  This "occurs when a domain is found in DNS using A
          records to multiple IP addresses, each of which has a very short
          Time-to-Live (TTL) value associated with it.  This means that the
          domain resolves to varying IP addresses over a short period of
          time."  (Quoted from [RFC6561], Section 1.1.5, with typo
          corrected) It is often used to deliver malware.  Because the
          addresses change so rapidly, it is difficult to ascertain all the
          hosts.  It should be noted that the technique also works with AAAA
          records, but such use is not frequently observed on the Internet
          as of this writing.

    Hoffman, et al.               Informational                    [Page 16]

    RFC 7719                     DNS Terminology               December 2015

    7.  Registration Model

       Registry:  The administrative operation of a zone that allows
          registration of names within that zone.  People often use this
          term to refer only to those organizations that perform
          registration in large delegation-centric zones (such as TLDs); but
          formally, whoever decides what data goes into a zone is the
          registry for that zone.  This definition of "registry" is from a
          DNS point of view; for some zones, the policies that determine
          what can go in the zone are decided by superior zones and not the
          registry operator.

       Registrant:  An individual or organization on whose behalf a name in
          a zone is registered by the registry.  In many zones, the registry
          and the registrant may be the same entity, but in TLDs they often
          are not.

       Registrar:  A service provider that acts as a go-between for
          registrants and registries.  Not all registrations require a
          registrar, though it is common to have registrars involved in
          registrations in TLDs.

       EPP:  The Extensible Provisioning Protocol (EPP), which is commonly
          used for communication of registration information between
          registries and registrars.  EPP is defined in [RFC5730].

       WHOIS:  A protocol specified in [RFC3912], often used for querying
          registry databases.  WHOIS data is frequently used to associate
          registration data (such as zone management contacts) with domain
          names.  The term "WHOIS data" is often used as a synonym for the
          registry database, even though that database may be served by
          different protocols, particularly RDAP.  The WHOIS protocol is
          also used with IP address registry data.

       RDAP:  The Registration Data Access Protocol, defined in [RFC7480],
          [RFC7481], [RFC7482], [RFC7483], [RFC7484], and [RFC7485].  The
          RDAP protocol and data format are meant as a replacement for
          WHOIS.

       DNS operator:  An entity responsible for running DNS servers.  For a
          zone's authoritative servers, the registrant may act as their own
          DNS operator, or their registrar may do it on their behalf, or
          they may use a third-party operator.  For some zones, the registry
          function is performed by the DNS operator plus other entities who
          decide about the allowed contents of the zone.

    Hoffman, et al.               Informational                    [Page 17]

    RFC 7719                     DNS Terminology               December 2015

    8.  General DNSSEC

       Most DNSSEC terms are defined in [RFC4033], [RFC4034], [RFC4035], and
       [RFC5155].  The terms that have caused confusion in the DNS community
       are highlighted here.

       DNSSEC-aware and DNSSEC-unaware:  These two terms, which are used in
          some RFCs, have not been formally defined.  However, Section 2 of
          [RFC4033] defines many types of resolvers and validators,
          including "non-validating security-aware stub resolver", "non-
          validating stub resolver", "security-aware name server",
          "security-aware recursive name server", "security-aware resolver",
          "security-aware stub resolver", and "security-oblivious
          'anything'".  (Note that the term "validating resolver", which is
          used in some places in DNSSEC-related documents, is also not
          defined.)

       Signed zone:  "A zone whose RRsets are signed and that contains
          properly constructed DNSKEY, Resource Record Signature (RRSIG),
          Next Secure (NSEC), and (optionally) DS records."  (Quoted from
          [RFC4033], Section 2.)  It has been noted in other contexts that
          the zone itself is not really signed, but all the relevant RRsets
          in the zone are signed.  Nevertheless, if a zone that should be
          signed contains any RRsets that are not signed (or opted out),
          those RRsets will be treated as bogus, so the whole zone needs to
          be handled in some way.

          It should also be noted that, since the publication of [RFC6840],
          NSEC records are no longer required for signed zones: a signed
          zone might include NSEC3 records instead.  [RFC7129] provides
          additional background commentary and some context for the NSEC and
          NSEC3 mechanisms used by DNSSEC to provide authenticated denial-
          of-existence responses.

       Unsigned zone:  Section 2 of [RFC4033] defines this as "a zone that
          is not signed".  Section 2 of [RFC4035] defines this as "A zone
          that does not include these records [properly constructed DNSKEY,
          Resource Record Signature (RRSIG), Next Secure (NSEC), and
          (optionally) DS records] according to the rules in this section".
          There is an important note at the end of Section 5.2 of [RFC4035]
          that defines an additional situation in which a zone is considered
          unsigned: "If the resolver does not support any of the algorithms
          listed in an authenticated DS RRset, then the resolver will not be
          able to verify the authentication path to the child zone.  In this
          case, the resolver SHOULD treat the child zone as if it were
          unsigned."

    Hoffman, et al.               Informational                    [Page 18]

    RFC 7719                     DNS Terminology               December 2015

       NSEC:  "The NSEC record allows a security-aware resolver to
          authenticate a negative reply for either name or type non-
          existence with the same mechanisms used to authenticate other DNS
          replies."  (Quoted from [RFC4033], Section 3.2.)  In short, an
          NSEC record provides authenticated denial of existence.

          "The NSEC resource record lists two separate things: the next
          owner name (in the canonical ordering of the zone) that contains
          authoritative data or a delegation point NS RRset, and the set of
          RR types present at the NSEC RR's owner name."  (Quoted from
          Section 4 of RFC 4034)

       NSEC3:  Like the NSEC record, the NSEC3 record also provides
          authenticated denial of existence; however, NSEC3 records mitigate
          against zone enumeration and support Opt-Out.  NSEC3 resource
          records are defined in [RFC5155].

          Note that [RFC6840] says that [RFC5155] "is now considered part of
          the DNS Security Document Family as described by Section 10 of
          [RFC4033]".  This means that some of the definitions from earlier
          RFCs that only talk about NSEC records should probably be
          considered to be talking about both NSEC and NSEC3.

       Opt-out:  "The Opt-Out Flag indicates whether this NSEC3 RR may cover
          unsigned delegations."  (Quoted from [RFC5155], Section 3.1.2.1.)
          Opt-out tackles the high costs of securing a delegation to an
          insecure zone.  When using Opt-Out, names that are an insecure
          delegation (and empty non-terminals that are only derived from
          insecure delegations) don't require an NSEC3 record or its
          corresponding RRSIG records.  Opt-Out NSEC3 records are not able
          to prove or deny the existence of the insecure delegations.
          (Adapted from [RFC7129], Section 5.1)

       Zone enumeration:  "The practice of discovering the full content of a
          zone via successive queries."  (Quoted from [RFC5155],
          Section 1.3.)  This is also sometimes called "zone walking".  Zone
          enumeration is different from zone content guessing where the
          guesser uses a large dictionary of possible labels and sends
          successive queries for them, or matches the contents of NSEC3
          records against such a dictionary.

       Key signing key (KSK):  DNSSEC keys that "only sign the apex DNSKEY
          RRset in a zone."(Quoted from [RFC6781], Section 3.1)

    Hoffman, et al.               Informational                    [Page 19]

    RFC 7719                     DNS Terminology               December 2015

       Zone signing key (ZSK):  "DNSSEC keys that can be used to sign all
          the RRsets in a zone that require signatures, other than the apex
          DNSKEY RRset."  (Quoted from [RFC6781], Section 3.1) Note that the
          roles KSK and ZSK are not mutually exclusive: a single key can be
          both KSK and ZSK at the same time.  Also note that a ZSK is
          sometimes used to sign the apex DNSKEY RRset.

       Combined signing key (CSK):  "In cases where the differentiation
          between the KSK and ZSK is not made, i.e., where keys have the
          role of both KSK and ZSK, we talk about a Single-Type Signing
          Scheme."  (Quoted from [RFC6781], Section 3.1) This is sometimes
          called a "combined signing key" or CSK.  It is operational
          practice, not protocol, that determines whether a particular key
          is a ZSK, a KSK, or a CSK.

       Secure Entry Point (SEP):  A flag in the DNSKEY RDATA that "can be
          used to distinguish between keys that are intended to be used as
          the secure entry point into the zone when building chains of
          trust, i.e., they are (to be) pointed to by parental DS RRs or
          configured as a trust anchor.  Therefore, it is suggested that the
          SEP flag be set on keys that are used as KSKs and not on keys that
          are used as ZSKs, while in those cases where a distinction between
          a KSK and ZSK is not made (i.e., for a Single-Type Signing
          Scheme), it is suggested that the SEP flag be set on all keys."
          (Quoted from [RFC6781], Section 3.2.3.)  Note that the SEP flag is
          only a hint, and its presence or absence may not be used to
          disqualify a given DNSKEY RR from use as a KSK or ZSK during
          validation.

       DNSSEC Policy (DP):  A statement that "sets forth the security
          requirements and standards to be implemented for a DNSSEC-signed
          zone."  (Quoted from [RFC6841], Section 2)

       DNSSEC Practice Statement (DPS):  "A practices disclosure document
          that may support and be a supplemental document to the DNSSEC
          Policy (if such exists), and it states how the management of a
          given zone implements procedures and controls at a high level."
          (Quoted from [RFC6841], Section 2)

    9.  DNSSEC States

       A validating resolver can determine that a response is in one of four
       states: secure, insecure, bogus, or indeterminate.  These states are
       defined in [RFC4033] and [RFC4035], although the two definitions
       differ a bit.  This document makes no effort to reconcile the two
       definitions, and takes no position as to whether they need to be
       reconciled.

    Hoffman, et al.               Informational                    [Page 20]

    RFC 7719                     DNS Terminology               December 2015

       Section 5 of [RFC4033] says:

          A validating resolver can determine the following 4 states:

          Secure: The validating resolver has a trust anchor, has a chain
             of trust, and is able to verify all the signatures in the
             response.

          Insecure: The validating resolver has a trust anchor, a chain
             of trust, and, at some delegation point, signed proof of the
             non-existence of a DS record.  This indicates that subsequent
             branches in the tree are provably insecure.  A validating
             resolver may have a local policy to mark parts of the domain
             space as insecure.

          Bogus: The validating resolver has a trust anchor and a secure
             delegation indicating that subsidiary data is signed, but
             the response fails to validate for some reason: missing
             signatures, expired signatures, signatures with unsupported
             algorithms, data missing that the relevant NSEC RR says
             should be present, and so forth.

          Indeterminate: There is no trust anchor that would indicate that a
             specific portion of the tree is secure.  This is the default
             operation mode.

       Section 4.3 of [RFC4035] says:

          A security-aware resolver must be able to distinguish between four
          cases:

          Secure: An RRset for which the resolver is able to build a chain
              of signed DNSKEY and DS RRs from a trusted security anchor to
              the RRset.  In this case, the RRset should be signed and is
              subject to signature validation, as described above.

          Insecure: An RRset for which the resolver knows that it has no
             chain of signed DNSKEY and DS RRs from any trusted starting
             point to the RRset.  This can occur when the target RRset lies
             in an unsigned zone or in a descendent [sic] of an unsigned
             zone.  In this case, the RRset may or may not be signed, but
             the resolver will not be able to verify the signature.

    Hoffman, et al.               Informational                    [Page 21]

    RFC 7719                     DNS Terminology               December 2015

          Bogus: An RRset for which the resolver believes that it ought to
             be able to establish a chain of trust but for which it is
             unable to do so, either due to signatures that for some reason
             fail to validate or due to missing data that the relevant
             DNSSEC RRs indicate should be present.  This case may indicate
             an attack but may also indicate a configuration error or some
             form of data corruption.

          Indeterminate: An RRset for which the resolver is not able to
             determine whether the RRset should be signed, as the resolver
             is not able to obtain the necessary DNSSEC RRs.  This can occur
             when the security-aware resolver is not able to contact
             security-aware name servers for the relevant zones.

    10.  Security Considerations

       These definitions do not change any security considerations for the
       DNS.

    11.  References

    11.1.  Normative References

       [RFC882]   Mockapetris, P., "Domain names: Concepts and facilities",
                  RFC 882, DOI 10.17487/RFC0882, November 1983,
                  <http://www.rfc-editor.org/info/rfc882>.

       [RFC1034]  Mockapetris, P., "Domain names - concepts and facilities",
                  STD 13, RFC 1034, DOI 10.17487/RFC1034, November 1987,
                  <http://www.rfc-editor.org/info/rfc1034>.

       [RFC1035]  Mockapetris, P., "Domain names - implementation and
                  specification", STD 13, RFC 1035, DOI 10.17487/RFC1035,
                  November 1987, <http://www.rfc-editor.org/info/rfc1035>.

       [RFC1123]  Braden, R., Ed., "Requirements for Internet Hosts -
                  Application and Support", STD 3, RFC 1123,
                  DOI 10.17487/RFC1123, October 1989,
                  <http://www.rfc-editor.org/info/rfc1123>.

       [RFC1996]  Vixie, P., "A Mechanism for Prompt Notification of Zone
                  Changes (DNS NOTIFY)", RFC 1996, DOI 10.17487/RFC1996,
                  August 1996, <http://www.rfc-editor.org/info/rfc1996>.

       [RFC2136]  Vixie, P., Ed., Thomson, S., Rekhter, Y., and J. Bound,
                  "Dynamic Updates in the Domain Name System (DNS UPDATE)",
                  RFC 2136, DOI 10.17487/RFC2136, April 1997,
                  <http://www.rfc-editor.org/info/rfc2136>.

    Hoffman, et al.               Informational                    [Page 22]

    RFC 7719                     DNS Terminology               December 2015

       [RFC2181]  Elz, R. and R. Bush, "Clarifications to the DNS
                  Specification", RFC 2181, DOI 10.17487/RFC2181, July 1997,
                  <http://www.rfc-editor.org/info/rfc2181>.

       [RFC2182]  Elz, R., Bush, R., Bradner, S., and M. Patton, "Selection
                  and Operation of Secondary DNS Servers", BCP 16, RFC 2182,
                  DOI 10.17487/RFC2182, July 1997,
                  <http://www.rfc-editor.org/info/rfc2182>.

       [RFC2308]  Andrews, M., "Negative Caching of DNS Queries (DNS
                  NCACHE)", RFC 2308, DOI 10.17487/RFC2308, March 1998,
                  <http://www.rfc-editor.org/info/rfc2308>.

       [RFC4033]  Arends, R., Austein, R., Larson, M., Massey, D., and S.
                  Rose, "DNS Security Introduction and Requirements",
                  RFC 4033, DOI 10.17487/RFC4033, March 2005,
                  <http://www.rfc-editor.org/info/rfc4033>.

       [RFC4034]  Arends, R., Austein, R., Larson, M., Massey, D., and S.
                  Rose, "Resource Records for the DNS Security Extensions",
                  RFC 4034, DOI 10.17487/RFC4034, March 2005,
                  <http://www.rfc-editor.org/info/rfc4034>.

       [RFC4035]  Arends, R., Austein, R., Larson, M., Massey, D., and S.
                  Rose, "Protocol Modifications for the DNS Security
                  Extensions", RFC 4035, DOI 10.17487/RFC4035, March 2005,
                  <http://www.rfc-editor.org/info/rfc4035>.

       [RFC4592]  Lewis, E., "The Role of Wildcards in the Domain Name
                  System", RFC 4592, DOI 10.17487/RFC4592, July 2006,
                  <http://www.rfc-editor.org/info/rfc4592>.

       [RFC5155]  Laurie, B., Sisson, G., Arends, R., and D. Blacka, "DNS
                  Security (DNSSEC) Hashed Authenticated Denial of
                  Existence", RFC 5155, DOI 10.17487/RFC5155, March 2008,
                  <http://www.rfc-editor.org/info/rfc5155>.

       [RFC5730]  Hollenbeck, S., "Extensible Provisioning Protocol (EPP)",
                  STD 69, RFC 5730, DOI 10.17487/RFC5730, August 2009,
                  <http://www.rfc-editor.org/info/rfc5730>.

       [RFC5936]  Lewis, E. and A. Hoenes, Ed., "DNS Zone Transfer Protocol
                  (AXFR)", RFC 5936, DOI 10.17487/RFC5936, June 2010,
                  <http://www.rfc-editor.org/info/rfc5936>.

    Hoffman, et al.               Informational                    [Page 23]

    RFC 7719                     DNS Terminology               December 2015

       [RFC6561]  Livingood, J., Mody, N., and M. O'Reirdan,
                  "Recommendations for the Remediation of Bots in ISP
                  Networks", RFC 6561, DOI 10.17487/RFC6561, March 2012,
                  <http://www.rfc-editor.org/info/rfc6561>.

       [RFC6672]  Rose, S. and W. Wijngaards, "DNAME Redirection in the
                  DNS", RFC 6672, DOI 10.17487/RFC6672, June 2012,
                  <http://www.rfc-editor.org/info/rfc6672>.

       [RFC6781]  Kolkman, O., Mekking, W., and R. Gieben, "DNSSEC
                  Operational Practices, Version 2", RFC 6781,
                  DOI 10.17487/RFC6781, December 2012,
                  <http://www.rfc-editor.org/info/rfc6781>.

       [RFC6840]  Weiler, S., Ed. and D. Blacka, Ed., "Clarifications and
                  Implementation Notes for DNS Security (DNSSEC)", RFC 6840,
                  DOI 10.17487/RFC6840, February 2013,
                  <http://www.rfc-editor.org/info/rfc6840>.

       [RFC6841]  Ljunggren, F., Eklund Lowinder, AM., and T. Okubo, "A
                  Framework for DNSSEC Policies and DNSSEC Practice
                  Statements", RFC 6841, DOI 10.17487/RFC6841, January 2013,
                  <http://www.rfc-editor.org/info/rfc6841>.

       [RFC6891]  Damas, J., Graff, M., and P. Vixie, "Extension Mechanisms
                  for DNS (EDNS(0))", STD 75, RFC 6891,
                  DOI 10.17487/RFC6891, April 2013,
                  <http://www.rfc-editor.org/info/rfc6891>.

       [RFC7344]  Kumari, W., Gudmundsson, O., and G. Barwood, "Automating
                  DNSSEC Delegation Trust Maintenance", RFC 7344,
                  DOI 10.17487/RFC7344, September 2014,
                  <http://www.rfc-editor.org/info/rfc7344>.

    11.2.  Informative References

       [DBOUND]   IETF, "Domain Boundaries (dbound) Working Group", 2015,
                  <https://datatracker.ietf.org/wg/dbound/charter/>.

       [RFC819]   Su, Z. and J. Postel, "The Domain Naming Convention for
                  Internet User Applications", RFC 819,
                  DOI 10.17487/RFC0819, August 1982,
                  <http://www.rfc-editor.org/info/rfc819>.

       [RFC952]   Harrenstien, K., Stahl, M., and E. Feinler, "DoD Internet
                  host table specification", RFC 952, DOI 10.17487/RFC0952,
                  October 1985, <http://www.rfc-editor.org/info/rfc952>.

    Hoffman, et al.               Informational                    [Page 24]

    RFC 7719                     DNS Terminology               December 2015

       [RFC1995]  Ohta, M., "Incremental Zone Transfer in DNS", RFC 1995,
                  DOI 10.17487/RFC1995, August 1996,
                  <http://www.rfc-editor.org/info/rfc1995>.

       [RFC3912]  Daigle, L., "WHOIS Protocol Specification", RFC 3912,
                  DOI 10.17487/RFC3912, September 2004,
                  <http://www.rfc-editor.org/info/rfc3912>.

       [RFC4641]  Kolkman, O. and R. Gieben, "DNSSEC Operational Practices",
                  RFC 4641, DOI 10.17487/RFC4641, September 2006,
                  <http://www.rfc-editor.org/info/rfc4641>.

       [RFC4697]  Larson, M. and P. Barber, "Observed DNS Resolution
                  Misbehavior", BCP 123, RFC 4697, DOI 10.17487/RFC4697,
                  October 2006, <http://www.rfc-editor.org/info/rfc4697>.

       [RFC4786]  Abley, J. and K. Lindqvist, "Operation of Anycast
                  Services", BCP 126, RFC 4786, DOI 10.17487/RFC4786,
                  December 2006, <http://www.rfc-editor.org/info/rfc4786>.

       [RFC4956]  Arends, R., Kosters, M., and D. Blacka, "DNS Security
                  (DNSSEC) Opt-In", RFC 4956, DOI 10.17487/RFC4956, July
                  2007, <http://www.rfc-editor.org/info/rfc4956>.

       [RFC5625]  Bellis, R., "DNS Proxy Implementation Guidelines",
                  BCP 152, RFC 5625, DOI 10.17487/RFC5625, August 2009,
                  <http://www.rfc-editor.org/info/rfc5625>.

       [RFC5890]  Klensin, J., "Internationalized Domain Names for
                  Applications (IDNA): Definitions and Document Framework",
                  RFC 5890, DOI 10.17487/RFC5890, August 2010,
                  <http://www.rfc-editor.org/info/rfc5890>.

       [RFC5891]  Klensin, J., "Internationalized Domain Names in
                  Applications (IDNA): Protocol", RFC 5891,
                  DOI 10.17487/RFC5891, August 2010,
                  <http://www.rfc-editor.org/info/rfc5891>.

       [RFC5892]  Faltstrom, P., Ed., "The Unicode Code Points and
                  Internationalized Domain Names for Applications (IDNA)",
                  RFC 5892, DOI 10.17487/RFC5892, August 2010,
                  <http://www.rfc-editor.org/info/rfc5892>.

       [RFC5893]  Alvestrand, H., Ed. and C. Karp, "Right-to-Left Scripts
                  for Internationalized Domain Names for Applications
                  (IDNA)", RFC 5893, DOI 10.17487/RFC5893, August 2010,
                  <http://www.rfc-editor.org/info/rfc5893>.

    Hoffman, et al.               Informational                    [Page 25]

    RFC 7719                     DNS Terminology               December 2015

       [RFC5894]  Klensin, J., "Internationalized Domain Names for
                  Applications (IDNA): Background, Explanation, and
                  Rationale", RFC 5894, DOI 10.17487/RFC5894, August 2010,
                  <http://www.rfc-editor.org/info/rfc5894>.

       [RFC6055]  Thaler, D., Klensin, J., and S. Cheshire, "IAB Thoughts on
                  Encodings for Internationalized Domain Names", RFC 6055,
                  DOI 10.17487/RFC6055, February 2011,
                  <http://www.rfc-editor.org/info/rfc6055>.

       [RFC6265]  Barth, A., "HTTP State Management Mechanism", RFC 6265,
                  DOI 10.17487/RFC6265, April 2011,
                  <http://www.rfc-editor.org/info/rfc6265>.

       [RFC6365]  Hoffman, P. and J. Klensin, "Terminology Used in
                  Internationalization in the IETF", BCP 166, RFC 6365,
                  DOI 10.17487/RFC6365, September 2011,
                  <http://www.rfc-editor.org/info/rfc6365>.

       [RFC7129]  Gieben, R. and W. Mekking, "Authenticated Denial of
                  Existence in the DNS", RFC 7129, DOI 10.17487/RFC7129,
                  February 2014, <http://www.rfc-editor.org/info/rfc7129>.

       [RFC7480]  Newton, A., Ellacott, B., and N. Kong, "HTTP Usage in the
                  Registration Data Access Protocol (RDAP)", RFC 7480,
                  DOI 10.17487/RFC7480, March 2015,
                  <http://www.rfc-editor.org/info/rfc7480>.

       [RFC7481]  Hollenbeck, S. and N. Kong, "Security Services for the
                  Registration Data Access Protocol (RDAP)", RFC 7481,
                  DOI 10.17487/RFC7481, March 2015,
                  <http://www.rfc-editor.org/info/rfc7481>.

       [RFC7482]  Newton, A. and S. Hollenbeck, "Registration Data Access
                  Protocol (RDAP) Query Format", RFC 7482,
                  DOI 10.17487/RFC7482, March 2015,
                  <http://www.rfc-editor.org/info/rfc7482>.

       [RFC7483]  Newton, A. and S. Hollenbeck, "JSON Responses for the
                  Registration Data Access Protocol (RDAP)", RFC 7483,
                  DOI 10.17487/RFC7483, March 2015,
                  <http://www.rfc-editor.org/info/rfc7483>.

       [RFC7484]  Blanchet, M., "Finding the Authoritative Registration Data
                  (RDAP) Service", RFC 7484, DOI 10.17487/RFC7484, March
                  2015, <http://www.rfc-editor.org/info/rfc7484>.

    Hoffman, et al.               Informational                    [Page 26]

    RFC 7719                     DNS Terminology               December 2015

       [RFC7485]  Zhou, L., Kong, N., Shen, S., Sheng, S., and A. Servin,
                  "Inventory and Analysis of WHOIS Registration Objects",
                  RFC 7485, DOI 10.17487/RFC7485, March 2015,
                  <http://www.rfc-editor.org/info/rfc7485>.

    Acknowledgements

       The authors gratefully acknowledge all of the authors of DNS-related
       RFCs that proceed this one.  Comments from Tony Finch, Stephane
       Bortzmeyer, Niall O'Reilly, Colm MacCarthaigh, Ray Bellis, John
       Kristoff, Robert Edmonds, Paul Wouters, Shumon Huque, Paul Ebersman,
       David Lawrence, Matthijs Mekking, Casey Deccio, Bob Harold, Ed Lewis,
       John Klensin, David Black, and many others in the DNSOP Working Group
       have helped shape this document.

    Authors' Addresses

       Paul Hoffman
       ICANN

       Email: paul.hoffman@icann.org

       Andrew Sullivan
       Dyn
       150 Dow Street, Tower 2
       Manchester, NH  03101
       United States

       Email: asullivan@dyn.com

       Kazunori Fujiwara
       Japan Registry Services Co., Ltd.
       Chiyoda First Bldg. East 13F, 3-8-1 Nishi-Kanda
       Chiyoda-ku, Tokyo  101-0065
       Japan

       Phone: +81 3 5215 8451
       Email: fujiwara@jprs.co.jp

    Hoffman, et al.               Informational                    [Page 27]