    Independent Submission                                          M. Chiba
    Request for Comments: 6812                                      A. Clemm
    Category: Informational                                        S. Medley
    ISSN: 2070-1721                                               J. Salowey
                                                                 S. Thombare
                                                                E. Yedavalli
                                                               Cisco Systems
                                                                January 2013

                     Cisco Service-Level Assurance Protocol

    Abstract

       Cisco's Service-Level Assurance Protocol (Cisco's SLA Protocol) is a
       Performance Measurement protocol that has been widely deployed.  The
       protocol is used to measure service-level parameters such as network
       latency, delay variation, and packet/frame loss.  This document
       describes the Cisco SLA Protocol Measurement-Type UDP-Measurement, to
       enable vendor interoperability.

    Status of This Memo

       This document is not an Internet Standards Track specification; it is
       published for informational purposes.

       This is a contribution to the RFC Series, independently of any other
       RFC stream.  The RFC Editor has chosen to publish this document at
       its discretion and makes no statement about its value for
       implementation or deployment.  Documents approved for publication by
       the RFC Editor are not a candidate for any level of Internet
       Standard; see Section 2 of RFC 5741.

       Information about the current status of this document, any errata,
       and how to provide feedback on it may be obtained at
       http://www.rfc-editor.org/info/rfc6812.

    Copyright Notice

       Copyright (c) 2013 IETF Trust and the persons identified as the
       document authors.  All rights reserved.

       This document is subject to BCP 78 and the IETF Trust's Legal
       Provisions Relating to IETF Documents
       (http://trustee.ietf.org/license-info) in effect on the date of
       publication of this document.  Please review these documents
       carefully, as they describe your rights and restrictions with respect
       to this document.

    Chiba, et al.                 Informational                     [Page 1]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    Table of Contents

       1.  Introduction . . . . . . . . . . . . . . . . . . . . . . . . .  3
       2.  Terminology  . . . . . . . . . . . . . . . . . . . . . . . . .  4
       3.  Protocol . . . . . . . . . . . . . . . . . . . . . . . . . . .  4
         3.1.  Control Phase  . . . . . . . . . . . . . . . . . . . . . .  6
           3.1.1.  Control-Request Message  . . . . . . . . . . . . . . .  7
             3.1.1.1.  Command-Header . . . . . . . . . . . . . . . . . .  8
             3.1.1.2.  CSLDs  . . . . . . . . . . . . . . . . . . . . . .  9
           3.1.2.  Control-Response Message . . . . . . . . . . . . . . . 15
         3.2.  Measurement Phase  . . . . . . . . . . . . . . . . . . . . 16
       4.  Implementation Notes . . . . . . . . . . . . . . . . . . . . . 19
       5.  Extensions . . . . . . . . . . . . . . . . . . . . . . . . . . 20
       6.  IANA Considerations  . . . . . . . . . . . . . . . . . . . . . 21
       7.  Security Considerations  . . . . . . . . . . . . . . . . . . . 24
         7.1.  Message Authentication . . . . . . . . . . . . . . . . . . 24
         7.2.  IPsec Considerations . . . . . . . . . . . . . . . . . . . 24
           7.2.1.  Control Traffic  . . . . . . . . . . . . . . . . . . . 24
           7.2.2.  Measurement Traffic  . . . . . . . . . . . . . . . . . 24
         7.3.  Replay Protection  . . . . . . . . . . . . . . . . . . . . 25
       8.  Acknowledgements . . . . . . . . . . . . . . . . . . . . . . . 25
       9.  References . . . . . . . . . . . . . . . . . . . . . . . . . . 25
         9.1.  Normative References . . . . . . . . . . . . . . . . . . . 25
         9.2.  Informative References . . . . . . . . . . . . . . . . . . 26

    Chiba, et al.                 Informational                     [Page 2]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    1.  Introduction

       Active network performance measurements are becoming critical data
       points for administrators monitoring the health of the network.  As
       service providers look to differentiate their offerings, performance
       measurement is increasingly becoming an important tool to monitor
       service-level guarantees and, in general, to monitor the health of a
       network.

       Performance metrics, both one-way and two-way, can be used for pre-
       deployment validation as well as for measuring in-band live network-
       performance characteristics.  It can be used to measure service
       levels in L2 and L3 networks as well as for applications running on
       top of L3.  Active performance measurements are gathered by analyzing
       synthetically generated request and response packets or frames.  This
       is in contrast to passive measurements that analyze live traffic
       flowing through a particular network element.

       There is a growing body of work on Performance Measurement standards
       that enable interoperability between different vendors' network
       elements by describing common measurement protocols as well as
       metrics.  The IETF has actively developed Standards Track documents
       on the subject, such as "A One-way Active Measurement Protocol
       (OWAMP)" [RFC4656] and "Two-Way Active Measurement Protocol (TWAMP)"
       [RFC5357].

       Cisco's SLA Protocol is another example of a Performance Measurement
       protocol that offers a rich set of measurement message types.  The
       measurement types can be classified as those that test connectivity
       (ping like) by providing round-trip or one-way latency measures, and
       those that provide a richer set of statistics including network
       jitter and packet or frame loss.  Each type of active measurement
       exchange mimics an actual protocol exchange.

       Cisco's SLA Protocol UDP-Measurement message exchanges, as covered in
       this document to enable interoperability, simulate a UDP application
       and can be used to simulate either Voice or Video traffic that is
       encoded in RTP frames within UDP envelopes.  The Measurement-Type
       UDP-Measurement message exchanges carry information that provide the
       ability to derive a robust set of statistics.

    Chiba, et al.                 Informational                     [Page 3]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    2.  Terminology

       The key words "MUST", "MUST NOT", "REQUIRED", "SHALL", "SHALL NOT",
       "SHOULD", "SHOULD NOT", "RECOMMENDED", "MAY", and "OPTIONAL" in this
       document are to be interpreted as described in RFC 2119 [RFC2119].

       +-------------+-----------------------------------------------------+
       | Term        | Description                                         |
       +-------------+-----------------------------------------------------+
       | Control     | A phase during which a Control-Request and Control- |
       | Phase       | Response are exchanged.                             |
       | ---------   | --------------------------                          |
       | L2          | OSI Data-Link Layer                                 |
       | ---------   | --------------------------                          |
       | L3          | OSI Network Layer                                   |
       | ---------   | --------------------------                          |
       | Measurement | Active Measurement Phase that is marked by a        |
       | Phase       | sequence of Measurement-Request and Measurement-    |
       |             | Response exchanges.                                 |
       | ---------   | --------------------------                          |
       | Metric      | A particular characteristic of the network data     |
       |             | traffic, for example, latency, jitter, packet or    |
       |             | frame loss.                                         |
       | ---------   | --------------------------                          |
       | Responder   | A network element that responds to a message.       |
       | ---------   | --------------------------                          |
       | RTP         | Real-time Transport Protocol                        |
       | ---------   | --------------------------                          |
       | Sender      | A network element that is the initiator of a        |
       |             | message exchange.                                   |
       | ---------   | --------------------------                          |
       | Service-    | This is the level of service that is agreed upon    |
       | Level       | between the Provider and the Customer.              |
       | ---------   | --------------------------                          |
       | UDP         | User Datagram Protocol                              |
       +-------------+-----------------------------------------------------+

    3.  Protocol

       The Cisco SLA Protocol consists of two distinct phases: the Control
       Phase and the Measurement Phase.  Each phase is comprised of
       information exchanged between a network element acting as the Sender
       and an element designated as the Responder.

       The Control Phase is the first phase of message exchanges and forms
       the base protocol.  This phase establishes the identity of the Sender
       and provides information for the Measurement Phase.  A single message
       pair of Control-Request and Control-Response marks this phase.  The

    Chiba, et al.                 Informational                     [Page 4]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       Sender initiates a Control-Request message that is acknowledged by
       the Responder with a Control-Response message.  The Control-Request
       may be sent multiple times if a Control-Response has not been
       received; the number of times the message is retried is configurable
       on the Sender element.

       The Measurement Phase forms the second phase and is comprised of a
       sequence of Measurement-Request and Measurement-Response messages.
       These messages may be exchanged as often as required.  Each
       Measurement-Request message is acknowledged by the Responder with a
       Measurement-Response message.

       The number and frequency with which messages are sent SHOULD be
       controlled by configuration on the Sender element, along with the
       waiting time for a Control-Response.

       The following sequence diagram depicts the message exchanges:

           +-+-+-+-+-+-+-+      Control-Request           +-+-+-+-+-+-+-+
           |             |                                |             |
           |    Sender   |                                |  Responder  |
           |             |                                |             |
           |             |                                |             |
           +-+-+-+-+-+-+-+                                +-+-+-+-+-+-+-+
                  |                                              |
                  |             Control-Request                  |
                  | -------------------------------------------->|
                  |                                              |
                  |             Control-Response                 |
                  |<---------------------------------------------|
                  |                                              |
                  |                                              |
                  |             Measurement-Request(1)           |
                  | -------------------------------------------->|
                  |                                              |
                  |             Measurement-Response(1)          |
                  |<---------------------------------------------|
                  |                                              |
                  .                                              .
                  .                                              .
                  .                                              .
                  .                                              .
                  .             Measurement-Request(n)           .
                  | -------------------------------------------->|
                  |                                              |
                  |             Measurement-Response(n)          |
                  |<---------------------------------------------|
                  |                                              |

    Chiba, et al.                 Informational                     [Page 5]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    3.1.  Control Phase

       The Control Phase begins with the Sender sending a Control-Request
       message to the Responder.  The Control-Request message is sent to UDP
       port 1167 on the Responder requesting that a Measurement Phase UDP
       port be opened and, in addition, indicates the duration for which the
       port needs to remain open.  The Responder replies by sending a
       Control-Response with an appropriate Status indicating Success when
       the Sender identity is verified and the requested UDP port was
       successfully opened.  In all other cases, a non-zero Status is
       returned in the Command-Header Status field.

       The sequence of exchanges is as indicated in the following diagram:

           +-+-+-+-+-+-+-+      Control-Request           +-+-+-+-+-+-+-+
           |             |------------------------------->|             |
           |    Sender   |                                |  Responder  |
           |             |      Control-Response          |             |
           |             |<-------------------------------|             |
           +-+-+-+-+-+-+-+                                +-+-+-+-+-+-+-+

    Chiba, et al.                 Informational                     [Page 6]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    3.1.1.  Control-Request Message

       The Control-Request message consists of a Command-Header followed by
       one or more Command, Status, Length and Data sections (henceforth
       known as CSLD).  At a minimum, there SHOULD be two CSLD sections, one
       of which is the authentication CSLD section and the other carries
       information for the Measurement Phase simulation type.

            0                   1                   2                   3
            0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                                                               |
           +                                                               +
           |                                                               |
           +                                                               +
           |                      Command-Header                           |
           +                                                               +
           |                                                               |
           +                                                               +
           |                                                               |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |     Command                   |           Status              |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                          Command-Length                       |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                                                               |
           .                                                               .
           .                          Data                                 .
           .                                                               .
           |                                                               |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |     Command                   |          Status               |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                         Command-Length                        |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                                                               |
           .                                                               .
           .                          Data                                 .
           .                                                               .
           |                                                               |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

    Chiba, et al.                 Informational                     [Page 7]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    3.1.1.1.  Command-Header

       The Command-Header is the first section of the Control-Request
       message and is depicted below:

            0                   1                   2                   3
            0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           | Version = 2   |     Reserved  |          Status               |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                         Sequence Number                       |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                         Total Length                          |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
           |                        Send Timestamp                         |
           +                                                               +
           |                                                               |
           +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

       The Command-Header fields hold the following meaning:

       +-----------+-----------+-------------------------------------------+
       | Field     | Size      | Description                               |
       |           | (bits)    |                                           |
       +-----------+-----------+-------------------------------------------+
       | Version   | 8         | Current version supported and is to be    |
       |           |           | set to 2.                                 |
       | --------- | --------- | --------------------------                |
       | Reserved  | 8         | Reserved field, MUST be set to 0.         |
       | --------- | --------- | --------------------------                |
       | Status    | 16        | Indicates success or failure for the      |
       |           |           | entire message.  In a Control-Request, the|
       |           |           | value of the Status field is ignored by   |
       |           |           | the receiver and SHOULD be set to 0.      |
       | --------- | --------- | --------------------------                |
       | Sequence  | 32        | Used to map requests to responses.  This  |
       | Number    |           | is a monotonically increasing number.     |
       |           |           | Implementations MAY reset the sequence    |
       |           |           | number to 0 after a reboot, and it SHOULD |
       |           |           | wrap around after all bits have been      |
       |           |           | exceeded.                                 |
       | --------- | --------- | --------------------------                |
       | Total     | 32        | Carries the total length of the Control   |
       | Length    |           | message in number of octets.              |
       | --------- | --------- | --------------------------                |

    Chiba, et al.                 Informational                     [Page 8]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       | --------- | --------- | --------------------------                |
       | Send      | 64        | This field is set to the time the command |
       | Timestamp |           | was submitted for transmission and is     |
       |           |           | updated for a response.  This field MAY   |
       |           |           | be used when security is of concern in    |
       |           |           | order to prevent replay attacks.  SHOULD  |
       |           |           | be updated when the response is sent.     |
       |           |           | When not being used, it MUST be set to all|
       |           |           | 0's.  The format is as given in RFC 5905. |
       +-----------+-----------+-------------------------------------------+

       The Sequence Number field MUST include a new number for each new
       request and is monotonically increasing.  When the Control-Request is
       to be retried, the sequence number MUST remain unchanged.

    3.1.1.2.  CSLDs

       The ordered list of the two CSLDs to be included along with the
       Command-Header are:

       o  The Authentication CSLD

       o  A Measurement-Type CSLD

       In this revision of the protocol, only a single Measurement-Type CSLD
       has been defined, the UDP-Measurement CSLD.  For future extensions,
       it is possible to add more Measurement-Type CSLDs.  For more details,
       see Section 5 on extensions.

    Chiba, et al.                 Informational                     [Page 9]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    3.1.1.2.1.  Authentication CSLD

       The Authentication CSLD provides message authentication and verifies
       that the requester knows the shared secret.  The following is the
       format for the Authentication CSLD:

           0                   1                   2                   3
           0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |           Command = 1         |            Status             |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                      Command-Length                           |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |     Mode      |   Reserved    |          Key Id               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          +                                                               +
          |                                                               |
          +                  Random Number                                +
          |                                                               |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          +                                                               +
          |                                                               |
          +                                                               +
          |                                                               |
          .                                                               .
          .                                                               .
          .                  Message Authentication Digest                .
          .                                                               .
          .                                                               .
          |                                                               |
          +                                                               +
          |                                                               |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

    Chiba, et al.                 Informational                    [Page 10]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       The fields for the Authentication CSLD have the following meaning:

       +----------------+-----------+--------------------------------------+
       | Field          | Size      | Description                          |
       |                | (bits)    |                                      |
       +----------------+-----------+--------------------------------------+
       | Command        | 16        | Indicates the CSLD is of type        |
       |                |           | Authentication.                      |
       | ---------      | --------- | --------------------------           |
       | Status         | 16        | Not used for a request and MUST be   |
       |                |           | set to 0.                            |
       | ---------      | --------- | --------------------------           |
       | Command-Length | 32        | Indicates the length of the CSLD in  |
       |                |           | octets.                              |
       | ---------      | --------- | --------------------------           |
       | Mode           | 8         | Indicates the type of authentication |
       |                |           | being used and is set as follows:    |
       |                |           | 0 - No Authentication,               |
       |                |           | 1 - SHA256 Authentication,           |
       |                |           | 2 - HMAC-SHA-256                     |
       | ---------      | --------- | --------------------------           |
       | Reserved       | 8         | This field is reserved for future    |
       |                |           | extensions and MUST be set to 0.     |
       | ---------      | --------- | --------------------------           |
       | Key ID         | 16        | Indicates the index number of the    |
       |                |           | shared secret to be used for         |
       |                |           | authenticating the Control-Request   |
       |                |           | message.                             |
       | ---------      | --------- | --------------------------           |
       | Random Number  | 128       | This field is to be unique over the  |
       |                |           | shared-secret life and is used to    |
       |                |           | make it difficult to predict the     |
       |                |           | shared secret via multiple packet    |
       |                |           | captures.  The value is reflected in |
       |                |           | a response message.  This field MAY  |
       |                |           | be used when security is of concern  |
       |                |           | and is useful to prevent dictionary  |
       |                |           | attacks.  When not being used, it    |
       |                |           | should be set to all 0's             |
       | ---------      | --------- | --------------------------           |
       | Message        | 256       | Contains the message authentication  |
       | Authentication |           | digest and is computed over the      |
       | Digest         |           | entire control packet, including this|
       |                |           | field set to all 0s.                 |
       +----------------+-----------+--------------------------------------+

    Chiba, et al.                 Informational                    [Page 11]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    3.1.1.2.2.  UDP-Measurement CSLD

       The UDP-Measurement CSLD indicates the Measurement-Type to be used
       during the Measurement Phase and specifies the addresses and UDP port
       to be opened as well as the duration that the port has to be kept
       open for the Measurement Phase.  The format of the CSLD is as
       follows:

           0                   1                   2                   3
           0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |           Command = 2         |            Status             |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                       Command-Length                          |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          | Address Type  |     Role      |          Reserved             |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                       Session Identifier                      |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          +                                                               +
          |                  Control Source Address                       |
          +                                                               +
          |                                                               |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          +                                                               +
          |                                                               |
          +                                                               +
          |                  Control Destination Address                  |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          +                                                               +
          |                                                               |
          +                                                               +
          |                  Measurement Source Address                   |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

    Chiba, et al.                 Informational                    [Page 12]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          +                                                               +
          |                                                               |
          +                                                               +
          |                  Measurement Destination Address              |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |  Control Source Port          |          Reserved             |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |  Measurement Source Port      | Measurement Destination Port  |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                         Duration                              |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

       Note: Duration is specified in milliseconds.

       The fields in the UDP-Measurement CSLD have the following meaning:

       +-------------+-----------+-----------------------------------------+
       | Field       | Size      | Description                             |
       |             | (bits)    |                                         |
       +-------------+-----------+-----------------------------------------+
       | Command     | 16        | Indicates that the CSLD is to simulate  |
       |             |           | UDP traffic measurements.               |
       | ---------   | --------- | --------------------------              |
       | Status      | 16        | Not used for a request and MUST be set  |
       |             |           | to 0.                                   |
       | ---------   | --------- | --------------------------              |
       | Command-    | 32        | Indicates the length of the CSLD in     |
       | Length      |           | octets.                                 |
       | ---------   | --------- | --------------------------              |
       | Address     | 8         | Indicates the address type and is set to|
       | Type        |           | one of the values in the "Cisco SLA     |
       |             |           | Protocol Address Family Registry":      |
       |             |           | 2 - IPv4 addresses, 3 - IPv6 addresses. |
       | ---------   | --------- | --------------------------              |
       | Role        | 8         | Indicates the role of the endpoint      |
       |             |           | receiving the Control message and is    |
       |             |           | set as follows: 1 - Responder.          |
       | ---------   | --------- | --------------------------              |
       | Reserved    | 16        | Reserved and MUST be set to 0.          |
       | ---------   | --------- | --------------------------              |

    Chiba, et al.                 Informational                    [Page 13]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       | ---------   | --------- | --------------------------              |
       | Session     | 32        | Carries a session identifier that is a  |
       | Identifier  |           | locally significant unique value to the |
       |             |           | originator of the message.  MUST be 0   |
       |             |           | when not specified.                     |
       | ---------   | --------- | --------------------------              |
       | Control     | 128       | Set to the address from which the       |
       | Source      |           | Sender initiates Control messages.  For |
       | Address     |           | IPv4 addresses, only the first 32 bits  |
       |             |           | are filled and the remaining bits MUST  |
       |             |           | be set to 0.                            |
       | ---------   | --------- | --------------------------              |
       | Control     | 128       | Set to the address on the Responder     |
       | Destination |           | where the Control message will be sent. |
       | Address     |           | For IPv4 addresses, only the first 32   |
       |             |           | bits are filled and the remaining bits  |
       |             |           | MUST be set to 0.                       |
       | ---------   | --------- | --------------------------              |
       | Measurement | 128       | Set to the address of the Sender from   |
       | Source      |           | where the measurement packets will      |
       | Address     |           | originate.  For IPv4 addresses, only the|
       |             |           | first 32 bits are filled and the        |
       |             |           | remaining bits MUST be set to 0.        |
       | ---------   | --------- | --------------------------              |
       | Measurement | 128       | Set to the address on the Responder     |
       | Destination |           | towards which the measurement packets   |
       | Address     |           | will be sent and is a way to identify   |
       |             |           | an ingress interface on the Responder.  |
       |             |           | For IPv4 addresses, only the first 32   |
       |             |           | bits are filled and the remaining bits  |
       |             |           | MUST be set to 0.                       |
       | ---------   | --------- | --------------------------              |
       | Control     | 16        | Indicates the port on the Sender from   |
       | Source Port |           | which the Control message is sent.  If  |
       |             |           | not set, the value should be derived    |
       |             |           | from the incoming packet.               |
       | ---------   | --------- | --------------------------              |
       | Reserved    | 16        | Reserved Field, MUST be set to 0.       |
       | ---------   | --------- | --------------------------              |
       | Measurement | 16        | Indicates the UDP Port on the Sender    |
       | Source Port |           | from which the measurement packets will |
       |             |           | be sent.                                |
       | ---------   | --------- | --------------------------              |
       | Measurement | 16        | Indicates the UDP Port on the Responder |
       | Destination |           | towards which the measurement packets   |
       | Port        |           | will be sent.                           |
       | ---------   | --------- | --------------------------              |

    Chiba, et al.                 Informational                    [Page 14]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       | ---------   | --------- | --------------------------              |
       | Duration    | 32        | This is the duration in milliseconds    |
       |             |           | that the port needs to be kept open for |
       |             |           | accepting Measurement Phase messages.   |
       |             |           | Measurement messages received after the |
       |             |           | duration MUST be ignored.               |
       +-------------+-----------+-----------------------------------------+

       Note: The source addresses are only indicative of identity of the
       originator and cannot be used as a destination address for responses
       in a NAT environment.

    3.1.2.  Control-Response Message

       In response to the Control-Request message, the network element
       designated the Responder sends back a Control-Response message that
       reflects the Command-Header with an updated Status field and includes
       the two CSLD sections that also carry updated Status fields.  Hence,
       the format is identical to the Control-Request message as described
       above.

       The following table shows the supported values of the Status fields:

       +-----------+-------------------------------------------------------+
       | Status    | Description                                           |
       | Value     |                                                       |
       +-----------+-------------------------------------------------------+
       | 0         | Success                                               |
       | --------- | --------------------------                            |
       | 1         | Fail - catch all                                      |
       | --------- | --------------------------                            |
       | 2         | Authentication Failure                                |
       | --------- | --------------------------                            |
       | 3         | Format error - sent when any CSLD type is not         |
       |           | recognized or any part of a CSLD has a value that is  |
       |           | not recognized                                        |
       | --------- | --------------------------                            |
       | 4         | Port in use - the UDP/TCP port is already being used  |
       |           | by some other application and cannot be reserved      |
       | --------- | --------------------------                            |
       | 5+        | Future extension and experimental values; refer to    |
       |           | the "Cisco SLA Protocol Status Types Registry" in the |
       |           | Considerations section (Section 6).                   |
       +-----------+-------------------------------------------------------+

       The Status field values are applicable to both Command-Header and
       CSLD sections.  In a Command-Header, the Status field indicates
       Success only if all the CSLD sections have their Status set to

    Chiba, et al.                 Informational                    [Page 15]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       Success.  The Command-Header Status field is set to non-zero
       otherwise.  The Status field in a Command-Header SHOULD only make use
       of status values 0 through 3, whereas CSLDs can also make use of
       other status values as applicable.  Future extensions MAY extend
       these values as appropriate.

       The Control-Response message, aside from updating the Status fields,
       SHOULD also update the Sent Timestamp (if used) in the Command-Header
       and the Message Authentication Digest in the Authentication CSLD.
       The Message Authentication Digest is computed in the same way as the
       Control-Request message.  The Random Number field MUST be reflected
       without modification.  The Session Identifier MAY be updated to
       reflect a locally significant unique value; it MUST be 0 if not
       specified.

    3.2.  Measurement Phase

       Upon receiving the Control-Response message with the Status set to
       Success, the second phase of the protocol, the Measurement Phase, is
       initiated.  In all other cases when the Status is not set to Success,
       no measurement traffic is initiated.  In the Measurement Phase, the
       Sender sends a stream of measurement messages.  The measurement
       message stream consists of packets or frames that are spaced a
       configured number of milliseconds apart.

          +-+-+-+-+-+-+-+      Measurement-Request(n)    +-+-+-+-+-+-+-+
          |             |------------------------------->|             |
          |    Sender   |                                |  Responder  |
          |             |      Measurement-Response(n)   |             |
          |             |<-------------------------------|             |
          +-+-+-+-+-+-+-+                                +-+-+-+-+-+-+-+

       The format of the measurement messages as defined by this document
       for UDP-Measurements is as shown below and is the same for the
       exchange in both directions.  That is, the format is the same when
       sent from the Sender to the Responder and when sent back from the
       Responder to the Sender with the only difference being the update of
       those fields that are designated with the Responder prefix; all other
       fields MUST remain unchanged.

    Chiba, et al.                 Informational                    [Page 16]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

           0                   1                   2                   3
           0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |   Measurement-Type = 3        |         Reserved              |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                    Sender Send Time                           |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                    Responder Receive Time                     |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                    Responder Send Time                        |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                    Sender Receive Time                        |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                    Sender Clock Offset                        |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                    Responder Clock Offset                     |
          +                                                               +
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                     Sender Sequence No.                       |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                     Responder Sequence No.                    |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
          |                                                               |
          .                                                               .
          .                          Data                                 .
          .                                                               .
          |                                                               |
          +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

    Chiba, et al.                 Informational                    [Page 17]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       The fields for the UDP-Measurement Measurement-Request have the
       following meaning:

       +-------------+-----------+-----------------------------------------+
       | Field       | Size      | Description                             |
       |             | (bits)    |                                         |
       +-------------+-----------+-----------------------------------------+
       | Measurement-| 16        | Carries the type of measurement being   |
       | Type        |           | performed; 1 - Reserved, 2 - Reserved,  |
       |             |           | 3 - UDP-Measurement                     |
       | ---------   | --------- | --------------------------              |
       | Reserved    | 16        | Reserved field and MUST be set to 0.    |
       | ---------   | --------- | --------------------------              |
       | Sender Send | 64        | Carries the timestamp when the          |
       | Time        |           | measurement message was submitted for   |
       |             |           | transmission by the Sender.             |
       | ---------   | --------- | --------------------------              |
       | Responder   | 64        | Carries the timestamp when the          |
       | Receive     |           | measurement message was received by     |
       | Time        |           | the Responder.                          |
       | ---------   | --------- | --------------------------              |
       | Responder   | 64        | Carries the timestamp when the          |
       | Send Time   |           | measurement message was submitted for   |
       |             |           | transmission by the Responder.  It MUST |
       |             |           | be 0 in the Sender-to-Responder         |
       |             |           | direction.                              |
       | ---------   | --------- | --------------------------              |
       | Sender      | 64        | Carries the timestamp when the Sender   |
       | Receive     |           | received the measurement message.  It   |
       | Time        |           | MUST be 0 in both directions on the     |
       |             |           | wire and is filled on the Sender side   |
       |             |           | as soon as the measurement message is   |
       |             |           | received.                               |
       | ---------   | --------- | --------------------------              |
       | Sender      | 64        | Gives an estimate of the Sender clock   |
       | Clock       |           | skew measured in seconds and fractional |
       | Offset      |           | seconds.                                |
       | ---------   | --------- | --------------------------              |
       | Responder   | 64        | Gives an estimate of the Responder      |
       | Clock       |           | clock skew measured in seconds and      |
       | Offset      |           | fractional seconds.                     |
       | ---------   | --------- | --------------------------              |
       | Sender      | 32        | The sequence number of the measurement  |
       | Sequence    |           | message on the Sender side.  This field |
       | Number      |           | is monotonically increasing and MAY     |
       |             |           | wrap around.                            |
       | ---------   | --------- | --------------------------              |

    Chiba, et al.                 Informational                    [Page 18]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       | ---------   | --------- | --------------------------              |
       | Responder   | 32        | The sequence number of the measurement  |
       | Sequence    |           | message on the Responder side.  This    |
       | Number      |           | field is monotonically increasing and   |
       |             |           | MAY wrap around.                        |
       | ---------   | --------- | --------------------------              |
       | Data        | 32 bit    | This field is used to pad up to the     |
       |             | aligned   | configured request data size.  The      |
       |             |           | minimum size for this field SHOULD be   |
       |             |           | 64 octets.                              |
       +-------------+-----------+-----------------------------------------+

       Note: All timestamps have the default format as described in RFC 5905
       [RFC5905] and is as follows: the first 32 bits represent the unsigned
       integer number of seconds elapsed since 0 h on 1 January 1900; the
       next 32 bits represent the fractional part of a second thereof.  The
       timestamp definition is also similar to that described in RFC 4656
       [RFC4656].

       In addition, the timestamp format used can be as described for the
       low-order 64 bits of the IEEE 1588-2008 (1588v2) Precision Time
       Protocol timestamp format [IEEE1588].  This truncated format consists
       of a 32-bit seconds field followed by a 32-bit nanoseconds field, and
       is the same as the IEEE 1588v1 timestamp format.  This timestamp
       definition is similar to the default timestamp specified in RFC 6374
       [RFC6374]

       Implementations MUST use only one of the two formats.  The chosen
       format is negotiated out-of-band between the endpoints or defaults to
       the format as defined in RFC 5905. [RFC5905]

    4.  Implementation Notes

       Responder implementations SHOULD support simultaneous measurements
       destined to a single port either from the same or a different Sender.
       For different measurement instances that originate from the same
       Sender, there MUST be a clear method for the Responder to distinguish
       the traffic, for example, per a unique 5-tuple of protocol, source
       address, source port, destination address, and destination port.

       A Control-Request that is received for the same Measurement-Type
       request as identified by the 5-tuples, for instance, SHOULD result in
       the resetting of the duration timer as well as the Responder sequence
       number.

       A Control Phase followed by the Measurement Phase can be repeated in
       order to have a continuous measurement over the entire lifetime of a
       device.

    Chiba, et al.                 Informational                    [Page 19]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       The Authentication CSLD MUST always be included.  The Random Number
       field is used to prevent dictionary attacks and is to be set to a
       random value in environments where security is a concern.

       An implementation MUST include the Random Number and Message
       Authentication fields when the mode is non-zero.  The fields MAY be
       included when the mode is set to 'No Authentication'; when present,
       they MUST be set to 0.  For the SHA256 authenticator mode, the shared
       secret is prepended to the Control message and the authentication
       algorithm is then run over the complete data including the shared
       secret.  The SHA256 mode is included for ease of implementation, and
       use of the HMAC variant is strongly recommended for stronger
       security.

       If the UDP port indicated in the UDP-Measurement CSLD is busy, the
       Responder MAY suggest an alternative port, in which case the Status
       of the UDP-Measurement CSLD MUST be set to Success.  The Sender MAY
       set a value of 0 in the field, in which case the Responder MAY choose
       to open a port and send that back along with the Status set to
       Success.  It should be noted that this behavior has security
       ramifications and the port needs to be chosen very carefully by the
       Responder.

       The measurement stream typically consists of packets or frames with a
       periodic inter-packet distribution.  The Sender need not wait for a
       Measurement-Response packet to arrive before sending another
       Measurement-Request packet; in many cases, it will not be possible to
       wait in order to maintain the desired inter-packet distribution.

       The default format for all timestamps is as specified in RFC 5905
       [RFC5905].

       All messages and fields within a message are assumed to be in network
       order.  In addition, all data fields are unsigned unless mentioned
       otherwise.

    5.  Extensions

       This section describes how the protocol can be extended to allow for
       additional functionality, such as new types of measurements.

       In order to allow for new types of measurements, additional
       Measurement-Type CSLDs can be defined to be carried within the
       Control-Request and Control-Response messages in place of the UDP-
       Measurement CSLD defined in this document.  The meaning and precise
       format of such a CSLD needs to be defined in a separate
       specification.  Such a specification will also need to describe the
       appropriate formats for the messages in the Measurement Phase.

    Chiba, et al.                 Informational                    [Page 20]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       In addition, the protocol can be extended by adding support for new
       values to registries defined in this document.

    6.  IANA Considerations

       The registries defined below are needed for the extensibility of the
       protocol.  In the registries, the terms 'Private Use' and
       'Experimental Use' have the same meaning as described in RFC 5226
       [RFC5226].

       Furthermore, for the following registries, the ranges designated
       "Unassigned" are governed by the policy 'RFC Required' as described
       in RFC 5226 [RFC5226].

       Cisco SLA Protocol Version Number Registry

                +-----------+------------------------+
                | Version   | Description            |
                +-----------+------------------------+
                | 0         | Reserved               |
                | 1         | Reserved               |
                | 2         | Version 2              |
                | 3 - 200   | Unassigned             |
                | 201 - 225 | Private Use            |
                | 226 - 255 | Experimental Use       |
                +-----------+------------------------+

       The version number should be changed only when the structure of the
       Command messages is different from the basic Command-Header and CSLD
       structure described in this document.

       Cisco SLA Protocol CSLD Command Registry

              +---------------+--------------------------+
              | CSLD Type     | Description              |
              +---------------+--------------------------+
              | 0             | Reserved                 |
              | 1             | Authentication CSLD      |
              | 2             | UDP-Measurement          |
              | 3 - 52        | Reserved                 |
              | 53 - 10239    | Unassigned               |
              | 10240 - 20479 | Private Use              |
              | 20480 - 65535 | Experimental Use         |
              +---------------+--------------------------+

       It is envisioned that future documents will provide their own
       Measurement-Type number and format of the Data portion.

    Chiba, et al.                 Informational                    [Page 21]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       Cisco SLA Protocol Authenticator Modes Registry

                +-----------+--------------------------+
                | Mode      | Description              |
                +-----------+--------------------------+
                | 0         | No Authentication        |
                | 1         | SHA256                   |
                | 2         | HMAC-SHA-256             |
                | 3 - 200   | Unassigned               |
                | 201 - 225 | Private Use              |
                | 226 - 255 | Experimental Use         |
                +-----------+--------------------------+

       Cisco SLA Protocol Roles Registry

                +-----------+--------------------------+
                | Role      | Description              |
                +-----------+--------------------------+
                | 0         | Reserved                 |
                | 1         | Sender                   |
                | 2         | Responder                |
                | 3 - 200   | Unassigned               |
                | 201 - 225 | Private Use              |
                | 226 - 255 | Experimental Use         |
                +-----------+--------------------------+

       Cisco SLA Protocol Measurement Type Registry

             +------------------+------------------------+
             | Measurement Type | Description            |
             +------------------+------------------------+
             | 0                | Reserved               |
             | 1                | Reserved               |
             | 2                | Reserved               |
             | 3                | UDP                    |
             | 4 - 52           | Reserved               |
             | 53-10239         | Unassigned             |
             | 10240 - 20479    | Private Use            |
             | 20480 - 65535    | Experimental Use       |
             +------------------+------------------------+

    Chiba, et al.                 Informational                    [Page 22]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       The following registry is also needed for the extensibility of the
       protocol.  However, the range designated "Unassigned" is governed by
       the policy 'First Come First Served' as described in RFC 5226
       [RFC5226].

       Cisco SLA Protocol Status Types Registry

       +-----------+-------------------------------------------------------+
       | Status    | Description                                           |
       +-----------+-------------------------------------------------------+
       | 0         | Success                                               |
       | --------- | --------------------------                            |
       | 1         | Fail - catch all                                      |
       | --------- | --------------------------                            |
       | 2         | Authentication failure                                |
       | --------- | --------------------------                            |
       | 3         | Format error - sent when any CSLD type is not         |
       |           | recognized or any part of a CSLD has a value that is  |
       |           | not recognized                                        |
       | --------- | --------------------------                            |
       | 4         | Port in use - the UDP/TCP port is already being used  |
       |           | by some other application and cannot be reserved      |
       | --------- | --------------------------                            |
       | 5 - 40959 | Unassigned                                            |
       | --------- | --------------------------                            |
       | 40960 -   | Experimental Use                                      |
       | 65535     |                                                       |
       +-----------+-------------------------------------------------------+

       Finally, the following registry is also needed for the extensibility
       of the protocol.  However, the range designated "Unassigned" is
       governed by the policy 'Specification Required' as described in RFC
       5226 [RFC5226].

       Cisco SLA Protocol Address Family Registry

                +--------------+------------------------+
                | Address Type | Description            |
                +--------------+------------------------+
                | 0            | Reserved               |
                | 1            | Reserved               |
                | 2            | IPv4                   |
                | 3            | IPv6                   |
                | 4 - 200      | Unassigned             |
                | 201 - 225    | Private Use            |
                | 226 - 255    | Experimental Use       |
                +--------------+------------------------+

    Chiba, et al.                 Informational                    [Page 23]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

    7.  Security Considerations

    7.1.  Message Authentication

       When the mode for the Authentication CSLD is set to 1, the Message
       Authentication Digest is generated using the SHA256 algorithm and is
       to be calculated over the entire packet including the Message
       Authentication Digest field, which MUST be set to all 0s.

       When the mode for the Authentication CSLD is set to 2, the Message
       Authentication Digest is generated using the HMAC-SHA-256 algorithm
       as described in RFC 4868 [RFC4868] and is to be calculated over the
       entire packet including the Message Authentication Digest field,
       which MUST be set to all 0s.

       When the mode field is set to 0, the Random Number and the Message
       Authentication Digest fields MAY be included; when present, they MUST
       be set to all 0s.

    7.2.  IPsec Considerations

       It is RECOMMENDED that IPsec be employed to afford better security.
       IPsec provides enhanced privacy as well as an automated key-
       distribution mechanism.  The recommendations below are similar to
       those in Section 2 of RFC 3579 [RFC3579].

    7.2.1.  Control Traffic

       For Senders implementing this specification, the IPsec policy would
       be "Initiate IPsec, from me to any, destination port UDP 1167".  This
       causes the Sender to initiate IPsec when sending control traffic to
       any Responder.  If some Responders contacted by the Sender do not
       support IPsec, then a more granular policy will be required, such as
       "Initiate IPsec, from me to IPsec-Capable-Responder, destination port
       UDP 1167".

       For Responders implementing this specification, the IPsec policy
       would be "Require IPsec, from any to me, destination port UDP 1167".
       This causes the Responder to require use of IPsec.  If some Sender
       does not support IPsec, then a more granular policy will be required:
       "Require IPsec, from IPsec-Capable-Sender to me".

    7.2.2.  Measurement Traffic

       As the Control Phase occurs before the Measurement Phase, it should
       be possible to build an IPsec Security Association once a successful
       Control-Response is received.

    Chiba, et al.                 Informational                    [Page 24]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       For Senders implementing this specification, the IPsec policy would
       be "Initiate IPsec, from me to negotiated address, destination is
       negotiated port".  This causes the Sender to initiate IPsec when
       sending measurement traffic to the Responder.  If some Responders
       contacted by the Sender do not support IPsec, then a more granular
       policy will be required, such as "Initiate IPsec, from me to IPsec-
       Capable-Responder, destination is negotiated port".

       For Responders implementing this specification, the IPsec policy
       would be "Require IPsec, from negotiated address to me, destination
       is negotiated port".  This causes the Responder to require use of
       IPsec.  If some Sender does not support IPsec, then a more granular
       policy will be required: "Require IPsec, from IPsec-Capable-Sender to
       me, destination is negotiated port".

    7.3.  Replay Protection

       For the Control messages, the originator of the message MAY choose to
       include a current value in the Sent Timestamp field indicating the
       time the message was submitted for transmission; otherwise, it MUST
       be set to 0.  The receiver of the message MAY choose to validate it
       if the timestamp is within an acceptable range.  The measurement
       traffic described in this document contains a timestamp to indicate
       the sent time and hence no new field is required.

    8.  Acknowledgements

       The authors wish to acknowledge the contributions of several key
       people who contributed to the current form of the document: Hanlin
       Fang, David Wang, Anantha Ramaiah, Max Pritikin, Malini Vijayamohan,
       and Susan Boyle.

    9.  References

    9.1.  Normative References

       [IEEE1588] IEEE, "1588-2008 Standard for a Precision Clock
                  Synchronization Protocol for Networked Measurement and
                  Control Systems", March 2008.

       [RFC2119]  Bradner, S., "Key words for use in RFCs to Indicate
                  Requirement Levels", BCP 14, RFC 2119, March 1997.

       [RFC4868]  Kelly, S. and S. Frankel, "Using HMAC-SHA-256, HMAC-
                  SHA-384, and HMAC-SHA-512 with IPsec", RFC 4868, May 2007.

    Chiba, et al.                 Informational                    [Page 25]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       [RFC5226]  Narten, T. and H. Alvestrand, "Guidelines for Writing an
                  IANA Considerations Section in RFCs", BCP 26, RFC 5226,
                  May 2008.

       [RFC5905]  Mills, D., Martin, J., Ed., Burbank, J., and W. Kasch,
                  "Network Time Protocol Version 4: Protocol and Algorithms
                  Specification", RFC 5905, June 2010.

    9.2.  Informative References

       [RFC3579]  Aboba, B. and P. Calhoun, "RADIUS (Remote Authentication
                  Dial In User Service) Support For Extensible
                  Authentication Protocol (EAP)", RFC 3579, September 2003.

       [RFC4656]  Shalunov, S., Teitelbaum, B., Karp, A., Boote, J., and M.
                  Zekauskas, "A One-way Active Measurement Protocol
                  (OWAMP)", RFC 4656, September 2006.

       [RFC5357]  Hedayat, K., Krzanowski, R., Morton, A., Yum, K., and J.
                  Babiarz, "A Two-Way Active Measurement Protocol (TWAMP)",
                  RFC 5357, October 2008.

       [RFC6374]  Frost, D. and S. Bryant, "Packet Loss and Delay
                  Measurement for MPLS Networks", RFC 6374, September 2011.

    Authors' Addresses

       Murtaza S. Chiba
       Cisco Systems
       170 West Tasman Drive
       San Jose,   95134
       USA

       Phone: 1-408-526-4000
       EMail: mchiba@cisco.com

       Alexander Clemm
       Cisco Systems
       170 West Tasman Drive
       San Jose,   95134
       USA

       Phone: 1-408-526-4000
       EMail: alex@cisco.com

    Chiba, et al.                 Informational                    [Page 26]

    RFC 6812         Cisco Service-Level Assurance Protocol     January 2013

       Steven Medley
       Cisco Systems
       170 West Tasman Drive
       San Jose,   95134
       USA

       Phone: 1-408-526-4000
       EMail: stmedley@cisco.com

       Joseph Salowey
       Cisco Systems
       170 West Tasman Drive
       San Jose,   95134
       USA

       Phone: 1-408-526-4000
       EMail: jsalowey@cisco.com

       Sudhir Thombare
       Cisco Systems
       170 West Tasman Drive
       San Jose,   95134
       USA

       Phone: 1-408-526-4000
       EMail: thombare@cisco.com

       Eshwar Yedavalli
       Cisco Systems
       170 West Tasman Drive
       San Jose,   95134
       USA

       Phone: 1-408-526-4000
       EMail: eshwar@cisco.com

    Chiba, et al.                 Informational                    [Page 27]